For 1990-2009 cars

## Driver or Passenger Seat Belt Buckle Replacement Lever Type Recliner

### Removal Procedure

1. Remove the screws (2) and the trim cover (1).
2. Remove the bolt (2) and the seat belt buckle (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt buckle (1) and secure with bolt (2) tighten to 38 N·m (28 lb ft).
2. Install the trim cover (1) and secure with the screws (2).

## Driver or Passenger Seat Belt Buckle Replacement Knob Type Recliner

### Removal Procedure

1. Remove the knob (1), screws (2) and the trim cover (3).
2. Remove the bolt (2) and the seat belt buckle (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt buckle (1) and secure with bolt (2) tighten to 38 N·m (28 lb ft).
2. Install the trim cover (3) and secure with the screws (2).
3. Install the knob (1).