For 1990-2009 cars

### Replacement Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel low cover.
3. Remove the screws and the lamp control module.
4. Disconnect the electrical connector.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lamp control module with the screws.
2. Connect the electrical connector.
3. Install the instrument panel low cover.
4. Connect the negative battery cable.