For 1990-2009 cars

## Front Floor Console Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the gearshift lever boot, if equipped.
3. Remove the screws from the floor console.
4. Remove the floor console cover.
5. Remove the parking brake cover.
6. Disconnect the electrical connector.
7. Remove the floor console.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the floor console with the screws.

Tighten
Tighten the floor console screws to 4 N·m (35 lb in).

3. Install the parking brake cover.
4. Install the floor console cover.
5. Install the gearshift lever boot, if equipped.
6. Connect the negative battery cable.

## Front Floor Console Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the gearshift lever boot.
3. Remove the screws from the floor console.
4. Disconnect the electrical connector.
5. Remove the floor console.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the floor console with the screws.

Tighten
Tighten the floor console screws to 4 N·m (35 lb in).

3. Install the gearshift lever boot.
4. Connect the negative battery cable.