For 1990-2009 cars

#### Special Tools

• | J 28647-B Engine Support Fixture

• | KM-6625 Flywheel Locking Device

### Removal Procedure

1. Install J 28647-B Engine Support Fixture .
2. Remove the automatic transmission. Refer to Transmission Replacement.
3. Install KM-6625 locking device (1) to block the crankshaft.
4. Install the transmission bolt with KM-6625 locking device .
5. Remove the flexible plate bolts (2).
6. Remove the flexible plate (1).

### Installation Procedure

1. Install the flexible plate (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the flexible plate bolts (2).

Tighten
Tighten the flexible plate bolts (2) to 35 N·m +30° +15° (25.8 lb ft +30° +15°).

3. Remove KM-6625 locking device (1) to block the crankshaft.
4. Install the automatic transmission. Refer to Transmission Replacement.
5. Remove J 28647-B Engine Support Fixture .