For 1990-2009 cars

## Rear Door Lock Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Disconnect the inside door handle and the lock rods.
4. Disconnect the outside door handle and the lock rods.
5. Remove the bolts and the guide rail.
6. Remove the screws and the lock.
7. Disconnect the electrical connector.
8. Disconnect the lock rods at the lock.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear door lock with the screws.

Tighten
Tighten the rear door lock screws to 8 N·m (71 lb in).

2. Connect the electrical connector.
3. Install the guide rail with the bolts.

Tighten
Tighten the guide rail bolts to 7 N·m (62 lb in).

4. Connect the outside door handle and the lock rods.
5. Connect the inside door handle and the lock rods.
6. Install the water deflector. Refer to Door Water Deflector Replacement .
7. Connect the negative battery cable.

## Rear Door Lock Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door water deflector. Refer to Door Water Deflector Replacement .
3. Disconnect the inside door handle and the lock rods.
4. Disconnect the outside door handle and the lock rods.
5. Remove the bolts and the guide rail.
6. Remove the screws and the lock.
7. Disconnect the electrical connector.
8. Disconnect the lock rods at the lock.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear door lock with the screws.

Tighten
Tighten the rear door lock screws to 8 N·m (71 lb in).

2. Connect the electrical connector.
3. Install the guide rail with the bolts.

Tighten
Tighten the guide rail bolts to 7 N·m (62 lb in).

4. Connect the outside door handle and the lock rods.
5. Connect the inside door handle and the lock rods.
6. Install the door water deflector. Refer to Door Water Deflector Replacement .
7. Connect the negative battery cable.