For 1990-2009 cars

### Removal Procedure

1. Remove the timing belt. Refer to Timing Belt Replacement.
2. Remove the camshaft sprocket bolt cap (4).
3. Remove the camshaft sprocket bolts (3).
4. Remove the camshaft sprockets (1, 2).

### Installation Procedure

Note: When installing the camshaft sprockets, the timing adjustment procedure must be accomplished. Refer to Timing Belt Replacement.

1. Install the camshaft sprockets (1, 2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the camshaft sprocket bolts (3).

Tighten
Tighten the camshaft sprocket bolts to 65 N·m (47.9 lb ft).

3. Install the camshaft sprocket bolt caps (4).

Tighten
Tighten the camshaft sprocket bolt cap to 50 N·m (36.8 lb ft).

4. Install the timing belt. Refer to Timing Belt Replacement.