For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the evaporative emission (EVAP) canister purge solenoid connector.
3. Disconnect the vacuum hoses from the EVAP canister purge solenoid.
4. Remove the EVAP canister purge solenoid from the intake manifold.

### Installation Procedure

1. Attach the EVAP canister purge solenoid to the intake manifold.
2. Connect the vacuum hoses to the EVAP canister purge solenoid.
3. Connect the EVAP canister purge solenoid connector.
4. Connect the negative battery cable.