For 1990-2009 cars

### Removal Procedure

Note: When removing the camshaft sprockets, the timing belt replacement procedure must be followed to ensure the camshafts and crankshaft are locked into position.

1. Remove the timing belt. Refer to Timing Belt Replacement.
2. Remove the camshaft intake sprocket bolt cap (4).
3. Remove the camshaft intake sprocket bolt (3).
4. Remove the camshaft intake sprocket with actuator (1).

### Installation Procedure

1. Install the camshaft intake sprocket (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the camshaft intake sprocket bolt (3).

Tighten
Tighten the camshaft sprocket bolt to 65 N·m (47.9 lb ft).

3. Install the camshaft intake sprocket bolt cap (4).

Tighten
Tighten the camshaft sprocket bolt cap to 50 N·m (36.8 lb ft).

4. Install the timing belt. Refer to Timing Belt Replacement.