For 1990-2009 cars

### Removal Procedure

1. Raise the hood and support it with the hood prop.
2. Remove the nuts and the wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Remove the air inlet grille screws and the 2-piece grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 2-piece grille and the air inlet grille screws.

Tighten
Tighten the air inlet grille screws to 2 N·m (18 lb in).

2. Install the nuts and the wiper arms. Refer to Windshield Wiper Arm Replacement .