For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint-to-Control Arm Nuts | 150 N·m | 111 lb ft
Ball Joint-to-Knuckle Nut | 55 N·m | 41 lb ft
Control Arm Front Mounting Bolt | 110 N·m | 81 lb ft
Control Arm Rear Mounting Bolts | 110 N·m | 81 lb ft
Crossmember Assembly Front to Body Nut | 150 N·m | 111 lb ft
Crossmember Assembly Rear to Body Nut | 150 N·m | 111 lb ft
Drive Axle-to-Hub Caulking Nut | 300 N·m | 221 lb ft
Engine Mounting Reaction Rod Bolts | 60 N·m | 44 lb ft
Knuckle Assembly to Front Strut Bolts | 100 N·m | 74 lb ft
Piston Rod Nut | 60 N·m | 44 lb ft
Power Steering Pipe Fittings | 22 N·m | 16 lb ft
Splash Shield-to-Steering Knuckle Screws | 4 N·m | 35 lb in
Stabilizer Shaft-to-Link Nut | 50 N·m | 37 lb ft
Strut Assembly-to-Body Nuts | 60 N·m | 44 lb ft
Tie Rod End Ball Joint Nut | 45 N·m | 33 lb ft
U-clamp Bolt | 25 N·m | 18 lb ft