For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the screws and the front speaker.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front speaker with the screws.

Tighten
Tighten the front speaker screws to 3.5 N·m (31 lb in).

3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Connect the negative battery cable.