For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rod clamp. Refer to Shift Linkage Adjustment.
3. Remove the console.
4. Remove the gearshift lever housing bolts and the gearshift lever housing.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the gearshift lever housing.
2. Install the gearshift lever housing bolts and tighten to 7 N·m (62 lb in).
3. Adjust the shift linkage. Refer to Shift Linkage Adjustment.
4. Install the console.
5. Connect the negative battery cable.