For 1990-2009 cars

## Remote Function Connector End Views Notchback

#### Remote Control Door Lock Receiver (RCDLR)/Theft Deterrent Control Module

Connector Part Information |

• | KET MG 611336

• | 26-Way F PCB Connector (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Arm Alarm Signal
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | PU | -- | Rear Compartment Lid Switch Signal
5 | OG/BK | -- | Rear Compartment Lid Ajar Switch Signal
6 | -- | -- | Not Used
7 | PK/D-BU | -- | Hood Ajar Switch Signal
8 | WH | -- | Door Ajar Signal
9 | L-BU | -- | Door Lock Control
10 | GY/D-GN | -- | Driver Door Lock Relay Lock Control
11 | YE | -- | Driver Door Lock Relay Unlock Control
12 | PU | -- | Door Latch Switch Signal
13 | D-BU | -- | Right Turn Signal Lamps Supply Voltage
14 | BN | -- | Rear Compartment Lid Switch Signal
15 | PK | -- | Ignition 1 Voltage
16 | -- | -- | Not Used
17 | BK/WH | -- | Serial Data
18 | L-GN | -- | Key In Ignition Switch Signal
19 | YE | -- | Security Indicator Control
20 | PU | -- | Door Latch Switch Signal
21-24 | -- | -- | Not Used
25 | RD/WH | -- | Battery Positive Voltage
26 | L-BU | -- | Left Turn Signal Lamps Supply Voltage

## Remote Function Connector End Views Hatchback

Table 1: | Hood Ajar Switch
Table 2: | Lock Cylinder Switch - Rear Compartment
Table 3: | Remote Control Door Lock Receiver (RCDLR)
Table 4: | Theft Deterrent Alarm
Table 5: | Theft Deterrent Control Module

#### Hood Ajar Switch

Connector Part Information |

• | KET MG 610392

• | 2-Way F Series Sealed (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/BK | 109 | Hood Ajar Switch Signal
2 | OG | 1440 | Battery Positive Voltage

#### Lock Cylinder Switch - Rear Compartment

Connector Part Information |

• | KET MG 610070

• | 2-Way F 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 737 | Rear Compartment Lid Ajar Switch Signal
2 | BK | 850 | Ground

#### Remote Control Door Lock Receiver (RCDLR)

Connector Part Information |

• | KET MG 611336

• | 26-Way F PCB Connector (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 261 | Arm Alarm Signal
2 | BK | 650 | Ground
3 | -- | -- | Not Used
4 | D-BU | 49 | Tamper Switch Signal (4-Door)
5 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
6 | -- | -- | Not Used
7 | BN/BK | 109 | Hood Ajar Switch Signal
8 | D-GN/WH | 157 | Courtesy Lamp Control
9 | GY | 195 | Door Lock Control
10 | GY/D-GN | 355 | Low Speed Cooling Fan Relay Control
11 | YE/D-GN | 356 | Driver Door Lock Relay Unlock Control
12 | D-BU | 49 | Tamper Switch Signal
13 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
14 | -- | -- | Not Used
15 | PK | 239 | Ignition 1 Voltage
16 | -- | -- | Not Used
17 | BK/WH | 2051 | Serial Data
18 | L-GN | 80 | Key In Ignition Switch Signal
19 | YE | 749 | Security Indicator Control
20 | D-BU | 49 | Tamper Switch Signal
21-24 | -- | -- | Not Used
25 | OG | 1340 | Battery Positive Voltage
26 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

#### Theft Deterrent Alarm

Connector Part Information |

• | KUM PB 625-02027

• | 2-Way F NMWP 04F-B Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 261 | Arm Alarm Signal
2 | BN | 641 | Ignition 3 Voltage

#### Theft Deterrent Control Module

Connector Part Information |

• | SD 35508-0700

• | 7-Way Connector F (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 239 | Ignition 1 Voltage
2 | OG | 240 | Battery Positive Voltage
3 | -- | -- | Not Used
4 | BK | 450 | Ground
5 | D-BU/WH | 1800 | Battery Positive Voltage
6 | BK/WH | 2051 | Serial Data
7 | YE | 749 | Security Indicator Control