For 1990-2009 cars

## Clock Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel center upper cover (1).
3. Remove the screws (2) and the clock (3).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the clock (3) with the screws (2) and tighten to 3 N·m (27 lb in).
2. Install the instrument panel center upper cover (1).
3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Clock Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel center upper cover.
3. Remove the screws and the clock.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the clock with the screws and tighten to 2.5 N·m (23 lb in).
2. Install the instrument panel center upper cover.
3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.