For 1990-2009 cars

### Removal Procedure

1. Loosen the air cleaner intake duct clamp at the air cleaner assembly.
2. Remove the air cleaner intake duct from the air cleaner assembly.
3. Remove the air cleaner assembly attachment bolts.
4. Remove the air cleaner assembly.

### Installation Procedure

1. Install the air cleaner assembly.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air cleaner assembly attachment bolts.

Tighten
Tighten the nut to 10 N·m (89 lb in).

3. Install the air cleaner intake duct to the air cleaner assembly.

Tighten
Tighten the air cleaner intake duct clamp to 3 N·m (27 lb in).