For 1990-2009 cars

1. Using a suitable puller, remove the tapered roller bearing from the transaxle case side.
2. Using a press, remove the counter driven gear.
3. Using a suitable puller, remove the tapered roller bearing.
4. Using a suitable puller, remove the outer tapered roller bearing race and shim from the transaxle case.
5. Using a suitable puller, remove the outer tapered roller bearing race from the transaxle housing.