For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat backs.
2. Remove the bolts that secure the rear seat backs to the hinges.
3. Remove the rear seat backs by pulling the seat hinge posts out of the front wheelhouse trim.

### Installation Procedure

1. Install the rear seat back by inserting the seat hinge posts into the front wheelhouse trim.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the seat backs to the hinges with the bolts and tighten to 25 N·m (18 lb ft).
3. Raise the rear seat backs in the upright position.