For 1990-2009 cars

#### Special Tools

• | J 28647-B Engine Support Fixture

• | KM-6625 Flywheel Locking Device

### Removal Procedure

1. Install J 28647-B Engine Support Fixture .
2. Remove the manual transmission. Refer to Transmission Replacement and Transmission Replacement.
3. Install KM-6625 locking device (1) to block the crankshaft.
4. Install the transmission bolt with KM-6625 locking device .
5. Remove the flywheel bolts.
6. Remove the flywheel (1).

### Installation Procedure

1. Install the flywheel (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the flywheel bolts.

Tighten
Tighten the flywheel bolts to 35 N·m +30° +15° (25.8 lb ft +30° +15°).

3. Remove KM-6625 locking device (1).
4. Install manual transaxle. Refer to Transmission Replacement and Transmission Replacement