For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the screws and the door pull bracket.
3. Remove the door seal trim.

### Installation Procedure

1. Install the door seal trim.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door pull bracket with the screws.

Tighten
Tighten the door pull bracket screws to 3.5 N·m (31 lb in).

3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .