For 1990-2009 cars

## Front Fog Lamp Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the nuts and the engine under cover.
3. Remove the bolts and the resonator.
4. Remove the nuts securing the fog lamp assembly.
5. Remove the fog lamp assembly.
6. Disconnect the electrical connector.
7. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the fog lamp with the screws and tighten to 5 N·m (44 lb in).
4. Install the resonator with the bolts.
5. Install the engine under cover with the bolts.
6. Connect the negative battery cable.

## Front Fog Lamp Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the nuts securing the fog lamp assembly.
3. Remove the fog lamp assembly.
4. Disconnect the electrical connector.
5. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Connect the electrical connector.
3. Install the fog lamp assembly.
4. Secure the fog lamp assembly with the nuts.
5. Connect the negative battery cable.