For 1990-2009 cars

### Removal Procedure

Caution: Refer to Electric Coolant Fan Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the cooling fan electrical connector(s) .
3. Remove the electric cooling fan mounting bolts.
4. Remove the electric cooling fan.

### Installation Procedure

1. Install the electric cooling fan(s).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the electric cooling fan mounting bolts.

Tighten
Tighten the electrical cooling fan mounting bolts to 4 N·m (35 lb in).

3. Connect the cooling fan electrical connector.