For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Gently pry up on the sun load sensor to remove it.
3. Secure the electrical connector to prevent it from falling beneath the dash.
4. Disconnect the electrical connector and remove the sun load sensor.

### Installation Procedure

1. Connect the electrical connector.
2. Insert and press the sun load sensor into position in the dash.
3. Connect the negative battery cable.