For 1990-2009 cars

1. Loosen the right and the left rod lock bolts.

Important: In this adjustment, the right and left tie rods must be equal in length.

2. Turn the right and the left tie rod adjusters to align the toe to 0 degrees ±10 minutes.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the tie rod lock bolts.

Tighten
Tighten the tie rod lock bolts to 64 N·m (47 lb ft).