For 1990-2009 cars

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1104 | Passenger Seat Occupant Classification System (OCS) Voltage Out of Range | SDM | DTC B1104
B1326 | Front End Sensor 1 Short to Ground | SDM | DTC B1326
B1327 | Front End Sensor 1 Short to Battery | SDM | DTC B1327
B1328 | Front End Sensor 1 Internal Electronic Failure | SDM | DTC B1328
B1329 | Front End Sensor 1 Invalid Serial Data Received | SDM | DTC B1329
B1330 | Incorrect Electronic Front End Sensor 1 Installed | SDM | DTC B1330
B1331 | Front End Sensor 2 Short to Ground | SDM | DTC B1331
B1332 | Front End Sensor 2 Short to Battery | SDM | DTC B1332
B1333 | Front End Sensor 2 Internal Electronic Failure | SDM | DTC B1333
B1334 | Front End Sensor 2 Invalid Serial Data Received | SDM | DTC B1334
B1335 | Incorrect Electronic Front End Sensor 2 Installed | SDM | DTC B1335
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Short to Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1440 | Passenger Seat Occupant Classification System (OCS) Short to Ground | SDM | DTC B1440
B1446 | Passenger Seat Occupant Classification System (OCS) Short to Battery | SDM | DTC B1446
B1447 | Passenger Seat Occupant Classification System (OCS) Sensor Circuit | SDM | DTC B1447
B1448 | Passenger Seat Occupant Classification System (OCS) Sensor | SDM | DTC B1448
B1449 | Passenger Seat Occupant Classification Sensor Communication | SDM | DTC B1449
B1450 | Incorrect Passenger Seat Occupant Classification Sensor Installed | SDM | DTC B1450
B1481 | Driver Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1481
B1482 | Driver Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1482
B1483 | Driver Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1483
B1484 | Driver Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1484
B1485 | Passenger Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1485
B1486 | Passenger Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1486
B1487 | Passenger Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1487
B1488 | Passenger Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1488
B1620 | ECU Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B1670 | Frontal Stage 2 Deployment Commanded | SDM | DTC B1670
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2501 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2501
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
C1101 | Battery Voltage High | EBCM | DTC C1101
C1102 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1102
C1200 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1200
C1201 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C1201
C1202 | Left Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1202
C1203 | Right Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1203
C1204 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C1204
C1205 | Right Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1205
C1206 | Left Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1206
C1207 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C1207
C1208 | Left Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1208
C1209 | Right Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1209
C1210 | ECU Malfunction | EBCM | DTC C1210
C1211 | Right Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1211
C1604 | ECU Malfunction | EBCM | DTC C1604
C2112 | Solenoid Valve Relay Circuit | EBCM | DTC C2112
C2402 | Pump Motor Circuit | EBCM | DTC C2402
P0016 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0016 or P0340
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030 or P0036
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0030 or P0036
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0068 | Throttle Body Air Flow Performance | ECM | DTC P0068
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM |

• | DTC P0106 for the 1.4L DOHC engine

• | DTC P0106 for the 1.4L SOHC engine

• | DTC P0106 for the 1.6L (L91) engine

P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC engine

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L (L91) engine

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC engine

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L (L91) engine

P0110 | Intake Air Temperature (IAT) Sensor Circuit | ECM | DTC P0110 or P0111
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0110 or P0111
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L (L91) engine

P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L (L91) engine

P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.5L engine

• | DTC P0117 or P0118 for the 1.6L (L91) engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.6L (L91) engine

P0118 | -- | ECM | DTC P0117 or P0118 for the 1.5L engine
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L (L91) engine

P0125 | Engine Coolant Temperature (ECT) Insufficient for Close Loop | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0132 | HO2S Circuit High Voltage Sensor 1 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0133 | HO2S Slow Response Sensor 1 | ECM |

• | DTC P0133 for the 1.2L engine

• | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine

• | DTC P0133, P1133, or P1134 for the 1.4L SOHC engine

• | DTC P0133 or P0139 for the 1.6L (L91) engine

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM |

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0134 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L (L91) engine

P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0133 or P0139
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM |

• | DTC P0140 for the 1.2L engine

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L (L91) engine

P0141 | HO2S Heater Performance Sensor 2 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L (L91) engine

P0171 | Fuel Trim System Lean | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L (L91) engine

P0172 | Fuel Trim System Rich | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L (L91) engine

P0201 | Injector 1 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0202 | Injector 2 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0203 | Injector 3 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0204 | Injector 4 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0217 | Engine Coolant Over Temperature | ECM | DTC P0217
P0222 | Idle Speed Control (ISP) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine
P0223 | Idle Speed Control (ISP) Motor Position Sensor Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L (L91) engine
P0300 | Engine Misfire Detected | ECM |

• | DTC P0300 for the 1.2L engine

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L (L91) engine

P0301 | Cylinder 1 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L (L91) engine

P0302 | Cylinder 2 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L (L91) engine

P0303 | Cylinder 3 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L (L91) engine

P0304 | Cylinder 4 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L (L91) engine

P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315
P0317 | Rough Road Sensing System Input Not Present | ECM | DTC P0317 for the 1.4L DOHC engine or DTC P0317 for the 1.4L SOHC engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 1.4L DOHC engine or DTC P0324 for the 1.6L (L91) engine
P0325 | Knock Sensor (KS) Circuit | ECM |

• | DTC P0325 for the 1.4L DOHC engine

• | DTC P0325 for the 1.4L SOHC engine

• | DTC P0325 for the 1.5L engine

• | DTC P0325 for the 1.6L (L91) engine

P0327 | Knock Sensor (KS) Circuit | ECM | DTC P0327 for the 1.2L engine or DTC P0327 for the 1.5L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0335 or P0336 for the 1.6L (L91) engine

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

• | DTC P0335 or P0336 for the 1.6L (L91) engine

P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016 or P0340
P0341 | Camshaft Position (CMP) Sensor Performance | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0342 | Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0351 | Ignition Coil 1 and 4 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L (L91) engine

P0352 | Ignition Coil 2 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L (L91) engine

P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L (L91) engine

P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L (L91) engine

P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L (L91) engine

P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L (L91) engine

P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L (L91) engine

P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L (L91) engine

P0420 | Catalyst System Low Efficiency | ECM |

• | DTC P0420 for the 1.2L engine

• | DTC P0420 for the 1.4L DOHC engine

• | DTC P0420 for the 1.4L SOHC engine

• | DTC P0420 for the 1.6L (L91) engine

P042E | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine or DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L (L91) engine
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM |

• | DTC P0443 for the 1.4L DOHC engine

• | DTC P0443 for the 1.4L SOHC engine

• | DTC P0443 for the 1.5L engine

P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0444 or P0445
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451 or P0454
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451 or P0454
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455
P0456 | Evaporative Emission (EVAP) System Very Small Leak Detected | ECM | DTC P0442 or P0456
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0458 or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0458 or P0459
P0496 | Evaporative Emission (EVAP) System Continuous Purge Flow | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Open | ECM | DTC P0498 or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Shorted | ECM | DTC P0498 or P0499
P0501 | Vehicle Speed Sensor (VSS) Circuit | ECM | DTC P0501
P0502 | Vehicle Speed Sensor (VSS) Circuit | ECM |

• | DTC P0502 for the 1.4L DOHC engine

• | DTC P0502 for the 1.4L SOHC engine

• | DTC P0502 for the 1.5L engine

• | DTC P0502 for the 1.6L (L91) engine

P0506 | Idle Speed Low | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L (L91) engine

P0507 | Idle Speed High | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L (L91) engine

P0510 | Idle Position Switch Circuit | ECM | DTC P0510
P0562 | System Voltage Low | TCM | DTC P0562
P0563 | System Voltage High | TCM | DTC P0563
P0600 | Control Module Internal Performance | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601 or P1790
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

TCM | DTC P0604
P0605 | Control Module Programming Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P0607 | Control Module Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P061B | Control Module Internal Performance | ECM | DTC P061B or P161B
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641 or P0651
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 or P1650 for the 1.2L engine or DTC P0650 for the 1.6L (L91) engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641 or P0651
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660 for the 1.4L DOHC engine or DTC P0660 for the 1.6L (L91) engine
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 1.4L DOHC engine

• | DTC P0700 for the 1.4L SOHC engine

• | DTC P0700 for the 1.6L (L91) engine

P0705 | Transmission Range Sensor Circuit | TCM | DTC P0705
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706
P0711 | Transmission Fluid Temperature Sensor (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature Sensor Low Input | TCM | DTC P0712
P0713 | Transmission Fluid Temperature Sensor Circuit High input | TCM | DTC P0713
P0717 | Input Speed Sensor - No Signal | TCM | DTC P0717
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0722
P0727 | Engine Speed Signal Circuit | TCM | DTC P0727
P0741 | Torque Converter Clutch (TCC) System-Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch Circuit Stuck On | TCM | DTC P0742
P0743 | Torque Converter Clutch Circuit Electrical | TCM | DTC P0743
P0748 | Pressure Control Solenoid Electrical | TCM | DTC P0748
P0751 | Shift Solenoid 1 Performance or Stuck Off | TCM | DTC P0751
P0752 | Shift Solenoid 1 Performance Stuck On | TCM | DTC P0752
P0753 | Shift Solenoid 1 Electrical | TCM | DTC P0753
P0756 | Shift Solenoid 2 Performance or Stuck Off | TCM | DTC P0756
P0757 | Shift Solenoid (SS) 2 Performance Stuck On | TCM | DTC P0757
P0758 | Shift Solenoid 2 Electrical | TCM | DTC P0758
P0785 | Shift Timing Solenoid | TCM | DTC P0785 or P1710
P0787 | Shift Timing Solenoid Low Voltage | TCM | DTC P0787
P0788 | Shift Timing Solenoid High Voltage | TCM | DTC P0788
P0834 | Clutch Pedal Switch Circuit Low Voltage | ECM | DTC P0834
P0835 | Clutch Pedal Switch Circuit High Voltage | ECM | DTC P0835
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0963
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0974
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0977
P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage | P1121 |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1133 | HO2S Insufficient Switching Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1134 | HO2S Transition Time Ratio Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1137 or P1166
P1138 | HO2S Circuit High Voltage During Diesel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1138 or P2297
P1166 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2 | ECM | DTC P1166 for the 1.4L DOHC engine or DTC P1137 or P1166 for the 1.6L (L91) engine
P1167 | HO2S Circuit High Voltage During Diesel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1167 for the 1.4L DOHC engine or DTC P1167 for the 1.4L SOHC engine
P1171 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1171 for the 1.4L DOHC engine or DTC P1171 for the 1.4L SOHC engine
P1230 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P1230 or P1231
P1231 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P1230 or P1231
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320
P1321 | Crankshaft Position (CKP) Reluctor Wheel Performance | ECM | DTC P1321
P1336 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1336 for the 1.4L DOHC engine or DTC P1336 for the 1.4L SOHC engine
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 or P1381
P1381 | Misfire Detected - No Communication With Brake Control Module | ECM | DTC P1380 or P1381 for the 1.4L DOHC engine or DTC P1380 or P1381 for the 1.4L SOHC engine
P1382 | Wheel Speed Sensor Circuit Performance | ECM | DTC P1382 or P1385
P1385 | Wheel Speed Sensor Circuit | ECM | DTC P1382 or P1385
P1390 | Left Driven Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396
P1391 | Rough Road Sensor Performance | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1392 | Rough Road Sensor Circuit Low Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1393 | Rough Road Sensor Circuit High Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1396 | Wheel Speed Sensor Circuit w/o ABS | ECM |

• | DTC P1390 or P1396 for the 1.2L engine

• | DTC P1396 or P1397 for the 1.4L DOHC engine

• | DTC P1396 or P1397 for the 1.6L (L91) engine

P1397 | Wheel Speed Sensor Circuit w/ABS | ECM | DTC P1396 or P1397 for the 1.4L DOHC engine or DTC P1396 or P1397 for the 1.6L (L91) engine
P1402 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L (L91) engine

P1403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404
P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

P1504 | Vehicle Speed Output Circuit 2 | ECM | DTC P1504
P1511 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P1511, P1512, or P1513
P1512 | Idle Speed Control (ISC) System | ECM | DTC P1511, P1512, or P1513
P1513 | Idle Speed Control (ISC) System Performance | ECM | DTC P1511, P1512, or P1513
P1516 | Throttle Actuator control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119
P1601 | Lost Communication with TCM | ECM |

• | DTC P1601 for the 1.4L DOHC engine

• | DTC P1601 for the 1.4L SOHC engine

• | DTC P1601 for the 1.5L engine

P1607 | -- | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611
P161B | Control Module Torque Performance | ECM | DTC P061B or P161B
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1650 or P1651
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1651 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1650 or P1651
P1660 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1660 or P1661
P1661 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1660 or P1661
P1701 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P1701 or P1792
P1702 | Engine Torque Signal Error | TCM | DTC P1702
P1710 | Timing Solenoid Electrical | TCM | DTC P0785 or P1710
P1781 | Engine Torque Signal Error | TCM | DTC P1781
P1790 | Internal Control Module Memory Checksum Error | TCM | DTC P0601 or P1790
P1791 | Throttle Position (TP) Sensor Circuit | TCM | DTC P1791
P1792 | Engine Coolant Signal | TCM | DTC P1701 or P1792
P2076 | Intake Manifold Tuning (IMT) Valve Position Sensor Performance | ECM | DTC P2076, P2077, or P2078
P2077 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078
P2078 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit High Voltage | ECM | DTC P2076, P2077, or P2078
P2101 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P2101, P2118, or P2119
P2101 | Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119
P2104 | Throttle Actuator Control (TAC) System - Forced Engine Idle | ECM | DTC P2104, P2105, P2106, or P2110
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2104, P2105, P2106, or P2110
P2106 | Throttle Control System Performance - Throttle Limitation Active | ECM | DTC P2104, P2105, P2106, or P2110
P2110 | Throttle Actuator Control (TAC) System - Forced Limited Engine Speed | ECM | DTC P2104, P2105, P2106, or P2110
P2118 | Idle Speed Control (ISC) System | ECM | DTC P2101, P2118, or P2119
P2119 | Idle Speed Control (ISC) System Performance | ECM | DTC P2101, P2118, or P2119
P2119 | Throttle Closed Position Performance | ECM | DTC P1516, P2101, or P2119
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2282 | Intake Manifold Air Leak | ECM | DTC P2282
P2297 | HO2S Circuit High Voltage during Diesel Fuel Cut-Off (DFCO) Sensor 2 | ECM | DTC P2297 for the 1.4L DOHC engine or DTC P1138 or P2297 for the 1.6L (L91) engine
P2610 | Control Module Ignition Off Timer Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L (L91) engine

P2769 | Torque Converter Clutch (TCC) Control Circuit Low Voltage | TCM | DTC P2769
P2770 | Torque Converter Clutch (TCC) Control Circuit High Voltage | TCM | DTC P2770
U0073 | High Speed Communication Bus | ECM/TCM | DTC U0073
U0401 | Invalid Data Received from ECM/PCM | TCM | DTC U0401
U2105 | CAN Bus Error | TCM | DTC U2105