For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electronic throttle control (ETC) connector from the accelerator pedal.
3. Remove the 3 accelerator pedal retaining nuts.
4. Remove the accelerator pedal.

### Installation Procedure

1. Position the accelerator pedal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 3 accelerator pedal retaining nuts.

Tighten
Tighten the accelerator pedal retaining nuts to 19 N·m (14 lb ft).

3. Connect the ETC connector to the accelerator pedal.
4. Connect the negative battery cable.