For 1990-2009 cars

### Removal Procedure

1. Raise the hood and support it with the hood prop.
2. Remove the nuts and the wiper arms. Refer to Windshield Wiper Arm Replacement.
3. Remove the air inlet grille screws and the 2-piece grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the 2-piece grille and the air inlet grille screws.

Tighten
Tighten the air inlet grille screws to 2 N·m (18 lb in).

2. Install the nuts and the wiper arms. Refer to Windshield Wiper Arm Replacement.