For 1990-2009 cars

## Air Conditioning Clutch Coil Removal V5 Compressor

#### Tools Required

• | J 8433-1 Puller Crossbar

• | J 8433-3 Forcing Screw

• | J 33023-A Puller Pilot

• | J 33025 Clutch Coil Puller Legs

### Disassembly Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
3. Remove the compressor. Refer to Air Conditioning Compressor Replacement .
4. Remove the clutch plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
5. Remove the clutch rotor and bearing. Refer to Clutch Rotor and Bearing Removal .
6. Mark the clutch coil terminal location on the compressor housing.
7. Install the J 33023-A (1) on the compressor housing. Also install the J 8433-1 (3) with the J 33025 (4).
8. Tighten the J 8433-3 (2) against the J 33023-A (1) to remove the clutch coil.

## Air Conditioning Clutch Coil Removal SP10 Compressor

1. Remove the clutch and drive assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
2. Remove the pulley and bearing assembly. Refer to Clutch Rotor and Bearing Removal .
3. Remove the coil retainer using the snap ring pliers (1).
4. Remove the coil and housing assembly.