For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement.
3. Disconnect the electrical connector.
4. Remove the motor retaining screws.
5. Remove the motor.

### Installation Procedure

1. Install the motor.
2. Install the motor retaining bolts and tighten.
3. Connect the electrical connector.
4. Install the instrument panel assembly. Refer to Instrument Panel Assembly Replacement
5. Connect the negative battery cable.