For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Gently pry off the interior courtesy lamp lens by inserting a screwdriver into the recess along the edge of the lens.
3. Remove the screws and the interior courtesy lamp housing from the headliner.
4. Disconnect the electrical connector.
5. Remove the bulb.

### Installation Procedure

1. Install a new bulb.
2. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the interior courtesy lamp housing to the headliner with the screws and tighten to 2.5 N·m (22 lb in).
4. Press the courtesy lamp lens onto the housing.
5. Connect the negative battery cable.