For 1990-2009 cars

The Data Display function contains lists of ABS and TCS data parameters. A brief description of all ABS and TCS data parameters available on the scan tool are listed below. The list is arranged in alphabetical order.

ABS Warning Indicator: The scan tool will display On or Off depending on the state of the ABS indicator.
Battery Voltage Signal: The scan tool displays 0 to 30 Volts. The voltage measured between the module's battery positive voltage circuit and ground circuit.
Brake Switch: The scan tool displays Applied or Released. The scan tool displays the state of the brake switch.
DRP Disabled: The scan tool will display Yes or No. This will indicate if the DRP has been disabled.
LF Inlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the LF inlet solenoid.
LF Outlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the LF outlet solenoid.
LF Wheel Speed Sensor: The scan tool displays 0-255 km/h (0-158 mph). The scan tool displays the actual speed of the left front wheel.
LR Inlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the LR inlet solenoid.
LR Outlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the actual state of the LR outlet solenoid.
LR Wheel Speed Sensor: The scan tool displays 0-255 km/h (0-158 mph). The scan tool displays the actual speed of the left rear wheel.
Pump Motor Command: The scan tool displays On or Off. The scan tool displays the commanded state of the pump motor.
Pump Motor Relay Command: The scan tool displays On or Off. The scan tool displays the commanded state of the pump motor relay.
RF Inlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the RF inlet solenoid.
RF Outlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the RF outlet solenoid.
RF Wheel Speed Sensor: The scan tool displays 0-255 km/h (0-158 mph). The scan tool displays the actual speed of the right front wheel.
RR Inlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the RR inlet solenoid.
RR Outlet Solenoid Command: The scan tool displays On or Off. The scan tool displays the commanded state of the RR outlet solenoid.
RR Wheel Speed Sensor: The scan tool displays 0-255 km/h (0-158 mph). The scan tool displays the actual speed of the right rear wheel.
Solenoid Relay Command: The scan tool displays On or Off. The scan tool displays the commanded state of the solenoid relay.