For 1990-2009 cars

## Washer Pump Replacement Typical

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the left front left wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the screws and the front wheel well splash shield.
4. Disconnect the electrical connector.
5. Disconnect the washer hose.
6. Remove the washer pump.

### Installation Procedure

1. Install the washer pump.
2. Connect the washer hose.
3. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the front wheel well splash shield with the screws.

Tighten
Tighten the front wheel well splash shield screws to 1.5 N·m (13 lb in).

5. Install the front left wheel. Refer to Tire and Wheel Removal and Installation.
6. Connect the negative battery cable.