For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the bolt and the seat belt buckle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt buckle and secure with bolt.

Tighten
Tighten the seat belt retractor bolt to 38 N·m (28 lb ft).

2. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.