For 1990-2009 cars

Connector 1: | X105 Engine Harness to TCM Harness (WHB)
Connector 2: | X105 TCM Harness to Engine Harness (Without WHB)
Connector 3: | X106 Engine Harness to Injector Harness (LMU)
Connector 4: | X204 I/P Harness to Engine Harness
Connector 5: | X205 I/P Harness to Engine Harness
Connector 6: | X206 TCM Harness to I/P Harness
Connector 7: | X207 Front Harness to I/P Harness (LHD)
Connector 8: | X208 Front Harness to I/P Harness (LHD)
Connector 9: | X209 Front Harness to I/P Harness
Connector 10: | X210 Roof Harness to Floor Harness
Connector 11: | X211 Front Harness to Floor Harness
Connector 12: | X212 I/P Harness to Floor Harness (LHD)
Connector 13: | X212 I/P Harness to Floor Harness (RHD)
Connector 14: | X213 I/P Harness to Floor Harness (LHD)
Connector 15: | X213 I/P Harness to Floor Harness (RHD)
Connector 16: | X214 I/P Harness to Floor Harness (LHD)
Connector 17: | X214 I/P Harness to Floor Harness (RHD)
Connector 18: | X215 Air Bag Harness to I/P Harness (C98)
Connector 19: | X216 Air Bag Harness to I/P Harness
Connector 20: | X217 I/P Harness to HVAC Harness (C68)
Connector 21: | X218 I/P Harness to Floor Harness (RHD)
Connector 22: | X219 I/P Harness to Floor Harness (RHD)
Connector 23: | X220 Front Harness to Floor Harness (RHD)
Connector 24: | X221 Front Harness to Floor Harness (RHD)
Connector 25: | X222 Cigar Lighter Harness to I/P Harness
Connector 26: | X223 I/P Harness to APP Jumper
Connector 27: | X351 Floor Harness to Driver Door Harness
Connector 28: | X361 Floor Harness to Passenger Door Harness
Connector 29: | X371 Floor Harness to Left Rear Door Harness
Connector 30: | X381 Floor Harness to Right Rear Door Harness
Connector 31: | X401 Tailgate Harness to Floor Harness (Hatchback)
Connector 32: | X401 Floor Harness to Trunk Harness (Notchback)
Connector 33: | C402 Tailgate Harness to Floor Harness (Hatchback)
Connector 34: | X402 Trunk Lid Harness to Floor Harness (Notchback)
Connector 35: | X403 Tailgate Extension Harness to Tailgate Harness (Hatchback)
Connector 36: | X404 Tailgate Harness to Tailgate Extension Harness (Hatchback)
Connector 37: | X405 Floor Harness to Left Tail Lamp Jumper (Hatchback without T9E)
Connector 38: | X406 Floor Harness to Right Tail Lamp Jumper (Hatchback without T9E)

### X105 Engine Harness to TCM Harness (WHB)

#### Connector Part Information

- OEM : 174257-2
- Service: N/A
- Description: 4-Way F J-Mark II Series, Tyco (BK)

#### Connector Part Information

- OEM: 174259-2
- Service: N/A
- Description: 4-Way M J-Mark II Series, Tyco (BK)

#### X105 Engine Harness to TCM Harness (WHB)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 710 | Class 2 Serial Data | 1 | YE | 710 | Class 2 Serial Data
2 | PU | 1807 | Class 2 Serial Data (Primary) | 2 | PU | 1807 | Class 2 Serial Data (Primary)
3 | BN | 323 | Shift Solenoid Feed | 3 | BN | 323 | Shift Solenoid Feed
4 | BK | 51 | Ground | 4 | BK | 50 | Ground

### X105 TCM Harness to Engine Harness (Without WHB)

#### Connector Part Information

- OEM: MG 641362-4
- Service: N/A
- Description: 3-Way F 090-II Series, KET (GY)

#### Connector Part Information

- OEM: MG 641359-4
- Service: N/A
- Description: 3-Way M 090-II Series, KET (GY)

#### X105 TCM Harness to Engine Harness (Without WHB)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 710 | Class 2 Serial Data | 1 | YE | 710 | Class 2 Serial Data
2 | PU | 1807 | Class 2 Serial Data (Primary) | 2 | PU | 1807 | Class 2 Serial Data (Primary)
3 | BK | 50 | Ground | 3 | BK | 51 | Ground

### X106 Engine Harness to Injector Harness (LMU)

#### Connector Part Information

- OEM : MG 610339
- Service: N/A
- Description: 8-Way F 090-II Series, Sealed KET (BK)

#### Connector Part Information

- OEM: MG 640341
- Service: N/A
- Description: 8-Way M 090-II Series, Sealed KET (BK)

#### X106 Engine Harness to Injector Harness (LMU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 1733 | Ignition 1 Voltage | 1 | BN | 1733 | Ignition 1 Voltage
2 | OG | 1733 | Ignition 1 Voltage | 2 | BN | 1733 | Ignition 1 Voltage
3 | OG | 1733 | Ignition 1 Voltage | 3 | BN | 1733 | Ignition 1 Voltage
4 | OG | 1733 | Ignition 1 Voltage | 4 | BN | 1733 | Ignition 1 Voltage
5 | L-BU/WH | 1747 | Low Reference | 5 | BN/RD | 1747 | Low Reference
6 | PK/BK | 1746 | Low Reference | 6 | L-GN/BK | 1746 | Low Reference
7 | L-GN/BK | 1745 | Low Reference | 7 | BN/WH | 1745 | Low Reference
8 | BN | 1744 | Low Reference | 8 | YE/D-BU | 1744 | Low Reference

### X204 I/P Harness to Engine Harness

#### Connector Part Information

- OEM: MG 611810-41
- Service: N/A
- Description: 18-Way F 090-II Series, KET (GY)

#### Connector Part Information

- OEM: MG 621807
- Service: N/A
- Description: 18-Way M 090-II, KET (WH)

#### X204 I/P Harness to Engine Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-GN/WH | 817 | Vehicle Speed Sensor Signal (MT) | 1 | L-BU | 817 | Vehicle Speed Sensor Signal (MT)
2 | WH | 121 | Engine Speed Signal (-WHB) | 2 | GY | 121 | Engine Speed Signal (-WHB)
3 | BN | 25 | Charge Indicator Signal (-WHB) | 3 | L-BU | 25 | Charge Indicator Signal (-WHB)
4 | BN/WH | 419 | MIL Control | 4 | BN | 419 | MIL Control
5 | BN | 841 | Ignition 3 Voltage (MT-WHB) | 5 | BN | 841 | Ignition 3 Voltage (MT-WHB)
6 | YE | 5 | Crank Voltage (MT-WHB) | 6 | YE | 5 | Crank Voltage (-WHB)
PU | 6 | Starter Solenoid Crank Voltage (AT-WHB)
7 | PU | 30 | Fuel Level Sensor Signal (-WHB) | 7 | PU | 30 | Fuel Level Sensor Signal (-WHB)
8 | D-BU | 1936 | Fuel Level Sensor Signal (Secondary) | 8 | GY | 1936 | Fuel Level Sensor Signal (Secondary)
9 | OG/BK | 1937 | Fuel Gage Sensor Ground | 9 | BN | 1937 | Low Rreference (-WHB)
BN | 1973 | Low Rreference (WHB)
10 | BN/BK | 1030 | Fuel Tank Pressure Sensor | 10 | L-BU | 1030 | Fuel Tank Pressure Sensor
11 | OG/BK | 1031 | Low Reference | 11 | L-BU | 1031 | Low Reference
12 | YE | 1578 | Fuel Temperature Signal | 12 | YE | 1578 | Fuel Temperature Signal
13 | BK/WH | 2051 | Serial Data (-WHB) | 13 | BK/WH | 2051 | Serial Data (-WHB)
14 | D-GN/WH | 762 | A/C Request Signal (-WHB) | 14 | D-GN/WH | 762 | A/C Request Signal (-WHB)
15 | L-GN | 24 | Backup Lamp Supply Voltaged (MT) | 15 | L-GN | 24 | Backup Lamp Supply Voltaged (MT)
16 | BN | 31 | Oil Pressure Indicator Control (-WHB) | 16 | D-GN | 31 | Oil Pressure Indicator Control (-WHB)
17 | D-GN | 135 | ECT Sensor Gauge Signal (-WHB) | 17 | WH | 135 | ECT Sensor Gauge Signal (-WHB)
18 | L-BU | 1937 | Low Reference | 18 | BN | 1937 | Low Reference (-WHB)
BN | 1973 | Low Reference (WHB)

### X205 I/P Harness to Engine Harness

#### Connector Part Information

- OEM: MG 611809
- Service: N/A
- Description: 18-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 621807
- Service: N/A
- Description:18-Way M 090-II, KET (WH)

#### X205 I/P Harness to Engine Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | 6338 | Clutch Pedal Position (CPP) Sensor Signal (WHB+M/T) | 1 | D-BU | 6338 | Clutch Pedal Position (CPP) Sensor Signal (WHB+M/T)
2 | RD/WH | 240 | Battery Positive Voltage | 2 | RD/WH | 240 | Battery Positive Voltage
3 | L-BU | 20 | Stop Lamp Supply Voltage | 3 | BN | 20 | Stop Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | OG | 7360 | Low Reference (MT+WHB) | 5 | OG | 7360 | Low Reference (MT+WHB)
6 | BN | 7361 | 5-Volt Reference (MT+WHB) | 6 | BN | 7361 | 5-Volt Reference (MT+WHB)
7 | L-BU | 1162 | APP Sensor 2 Signal | 7 | WH | 1162 | APP Sensor 2 Signal
8 | GY | 474 | 5-Volt Reference | 8 | GY | 474 | 5-Volt Reference
9 | GY | 596 | 5-Volt Reference | 9 | GY | 596 | 5-Volt Reference
10 | D-BU | 1161 | APP Sensor 1 Signal | 10 | D-BU | 1161 | APP Sensor 1 Signal
11 | OG/BK | 645 | Low Reference | 11 | YE | 645 | Low Reference
12 | BN | 718 | Low Reference | 12 | D-GN/WH | 718 | Low Reference
13 | YE | 111 | Vehicle Wake Up Signal (WHB) | 13 | BN | 7007 | Vehicle Wake Up Signal (WHB)
14 | PU | 1807 | Class 2 Serial Data (Primary) | 14 | PU | 1807 | Class 2 Serial Data (Primary)
15 | YE | 710 | Class 2 Serial Data | 15 | YE | 710 | Class 2 Serial Data
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | OG | 551 | Oil Level Sensor Signal (NT4) | 17 | OG | 551 | Oil Level Sensor Signal (NT4)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used

### X206 TCM Harness to I/P Harness

#### Connector Part Information

- OEM: HS015-10125
- Service: N/A
- Description: 10-Way F 090 CS Series, KUM (GY)

#### Connector Part Information

- OEM: HS011-10125
- Service: N/A
- Description: 10-Way M 090 CS Series, KUM (GY)

#### X206 TCM Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 440 | Battery Positive Voltage | 1 | RD/WH | 440 | Battery Positive Voltage
2 | BN | 323 | Shift Solenoid Feed | 2 | BN | 323 | Shift Solenoid Feed (-WHB)
BN | 323 | Shift Solenoid Feed (WHB)
3 | L-GN | 24 | Back-Up Lamp Feed | 3 | L-GN | 24 | Back-Up Lamp Feed
L-GN | 24 | Back-Up Lamp Feed
4 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage (-WHB) | 4 | GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage (-WHB)
YE | 710 | Class 2 Serial Data (WHB) | YE | 710 | Class 2 Serial Data (WHB)
5 | L-BU | 20 | Stop Lamp Supply Voltage | 5 | L-BU | 20 | Stop Lamp Supply Voltage
6 | BK/WH | 2051 | Serial Data (-WHB) | 6 | BK/WH | 2051 | Serial Data (-WHB)
YE | 111 | Vehicle Wake Up Signal (WHB) | YE | 111 | Vehicle Wake Up Signal (WHB)
7 | D-GN/WH | 817 | Vehicle Speed Signal | 7 | D-GN/WH | 817 | Vehicle Speed Signal (-WHB)
D-GN/WH | 817 | Vehicle Speed Signal
8 | PK | 841 | Ignition 2 Voltage (-WHB) | 8 | BN | 841 | Ignition 2 Voltage (-WHB)
9 | PK | 239 | Ignition 1 Voltage | 9 | PK | 239 | Ignition 1 Voltage
PK | 239 | Ignition 1 Voltage
10 | YE | 1481 | Transmission Auxiliary Hold Signal (-WHB) | 10 | YE | 1481 | Transmission Auxiliary Hold Signal (-WHB)
PU | 1807 | Class 2 Serial Data (Primary) (WHB) | PU | 1807 | Class 2 Serial Data (Primary) (WHB)

### X207 Front Harness to I/P Harness (LHD)

#### Connector Part Information

- OEM: MG 653012-4
- Service: N/A
- Description: 12-Way F 090-II Series, KET (GY)

#### Connector Part Information

- OEM: MG 643009-4
- Service: N/A
- Description: 12-Way M 090-II Series, KET (GY)

#### X207 Front Harness to I/P Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | 7002 | Run Relay Out (WHB) | 1 | D-BU | 7002 | Run Relay Out (WHB)
2 | YE | 1769 | Fog Lamp Switch Supply Voltage (T96) | 2 | YE | 1769 | Fog Lamp Switch Supply Voltage (T96)
3 | D-GN/WH | 1317 | Fog Lamp Relay Control (T96) | 3 | D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
4 | L-GN/BK | 867 | ABS Indicator Failure Control (JM4) | 4 | L-GN | 867 | ABS Indicator Failure Control
BK | 50 | Ground (-JM4)
5 | BK/WH | 2051 | Serial Data (JM4) | 5 | BK/WH | 2051 | Serial Data
6 | YE/BK | 6169 | Low Reference (WHB) | 6 | YE/BK | 6169 | Low Reference (WHB)
D-BU | 732 | Evaporator Temperature Sensor Signal (-LDT/WHB) | D-BU | 732 | Evaporator Temperature Sensor Signal (-LDT/WHB)
7 | YE | 6168 | SIR Front End Sensor Signal - Left (WHB) | 7 | YE | 6168 | SIR Front End Sensor Signal - Left (WHB)
L-BU | 733 | Low Reference (-LDT/WHB) | L-BU | 733 | Low Reference (-LDT/WHB)
8 | L-GN | 6777 | Low Reference (WHB) | 8 | L-GN | 6777 | Low Reference (WHB)
YE | 61 | Low Reference (U68) | YE | 61 | Low Reference (-WHB)
9 | BN/WH | 6776 | SIR Front End Sensor Signal - Right (WHB) | 9 | BN/WH | 6776 | SIR Front End Sensor Signal - Right (WHB)
L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (U68-WHB) | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (-WHB)
10 | BK | 50 | Ground (-JM4) | 10 | BK | 50 | Ground
11 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (TR6) | 11 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (TR6)
YE | 61 | Low Reference (WHB) | YE | 61 | Low Reference (WHB)
12 | PK/BK | 109 | Hood Ajar Switch Signal (UA5) | 12 | PK/BK | 109 | Hood Ajar Switch Signal (UA5)

### X208 Front Harness to I/P Harness (LHD)

#### Connector Part Information

- OEM: PK 146-22107
- Service: N/A
- Description: 22-Way F (OG)

#### Connector Part Information

- OEM: PK 142-22107
- Service: N/A
- Description: 22-Way M (OG)

#### X208 Front Harness to I/P Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 92 | Windshield Wiper Motor High Speed | 1 | PU | 92 | Windshield Wiper Motor High Speed
2 | BN | 96 | Windshield Wiper Switch Pulse Delay Signal | 2 | BN | 96 | Windshield Wiper Switch Pulse Delay Signal
3 | PK | 94 | Windshield Washer Switch Signal | 3 | PK | 94 | Windshield Washer Switch Signal
PK | 94 | Windshield Washer Switch Signal
4 | RD/WH | 440 | Battery Positive Voltage | 4 | RD/WH | 1440 | Battery Positive Voltage
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | BN/WH | 309 | Right Park Lamp Supply Voltage | 6 | BN/WH | 309 | Right Park Lamp Supply Voltage
7 | BN | 33 | Brake Warning Indicator Control | 7 | BN/WH | 33 | Brake Warning Indicator Control
8 | BN | 28 | Horn Relay Control | 8 | BN | 28 | Horn Relay Control
BN | 28 | Horn Relay Control
9 | WH | 352 | Headlamp Relay Coil Supply Voltage | 9 | WH | 352 | Headlamp Relay Coil Supply Voltage
10 | PU | 638 | Power Window Motor Driver Down Control | 10 | PU | 638 | Power Window Motor Driver Down Control
11 | D-GN | 95 | Windshield Washer Switch Signal | 11 | D-GN | 95 | Windshield Washer Switch Signal
12 | PK | 639 | Ignition 1 Voltage | 12 | PK | 639 | Ignition 1 Voltage
13 | L-GN/BK | 392 | Rear Window Washer Pump Control | 13 | L-GN/BK | 392 | Rear Window Washer Pump Control
L-GN/BK | 392 | Rear Window Washer Pump Control (hatchback)
14 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | 14 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
15 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 15 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
16 | PK | 539 | Ignition 1 Voltage | 16 | PK | 539 | Ignition 1 Voltage
PK | 539 | Ignition 1 Voltage (L95/LV8/LXT)
17 | PK/BK | 1739 | Ignition 1 Voltage (L95/LV8/LXT) | 17 | PK | 1739 | Ignition 1 Voltage (-WHB)
L-GN/BK | 735 | Low Reference (WHB) | BK | 735 | Low Reference (WHB)
18 | RD/WH | 440 | Battery Positive Voltage | 18 | RD/WH | 440 | Battery Positive Voltage (AT)
19 | YE | 712 | Left Headlamp Low Beam Supply Voltage | 19 | YE | 712 | Left Headlamp Low Beam Supply Voltage
20 | RD/WH | 580 | Battery Positive Voltage (WHB) | 20 | RD/WH | 580 | Battery Positive Voltage (WHB)
21 | L-BU | 1346 | Headlamp Supply Voltage | 21 | L-BU | 1346 | Headlamp Supply Voltage
22 | WH | 1080 | Park Lamp Relay Control | 22 | WH | 1080 | Park Lamp Relay Control

### X209 Front Harness to I/P Harness

#### Connector Part Information

- OEM: MG 651926-5
- Service: N/A
- Description: 4-Way F 312-II Series, KET (BK)

#### Connector Part Information

- OEM: MG 641928-5
- Service: N/A
- Description: 4-Way M 312-II Series, KET (BK)

#### X209 Front Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/BK | 142 | Battery Positive Voltage | 1 | RD/BK | 142 | Battery Positive Voltage
2 | RD/BK | 42 | Battery Positive Voltage | 2 | RD/BK | 42 | Battery Positive Voltage (-WHB)
OG | 300 | Ignition 3 Voltage (WHB)
3 | RD/BK | 242 | Battery Positive Voltage | 3 | RD/BK | 242 | Battery Positive Voltage
4 | L-GN/BK | 440 | Battery Positive Voltage (RHD) | 4 | L-GN/BK | 440 | Battery Positive Voltage (RHD)

### X210 Roof Harness to Floor Harness

#### Connector Part Information

- OEM: 936092-4
- Service: N/A
- Description: 10-Way F 090-III Series, AMP (BN)

#### Connector Part Information

- OEM: 936129-4
- Service: N/A
- Description: 10-Way M 090-III Series, AMP (BN)

#### X210 Roof Harness to Floor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 450 | Ground (CF5) | 1 | BK | 450 | Ground
2 | BN | 641 | Ignition 3 Voltage (CF5) | 2 | BN | 641 | Ignition 3 Voltage
3 | RD/WH | 640 | Battery Positive Voltage (CF5) | 3 | RD/WH | 640 | Battery Positive Voltage
4 | GY | 118 | Left Front Speaker Output (-) (UW6) | 4 | GY | 118 | Left Front Speaker Output (-)
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | GY | 157 | Courtesy Lamp Control | 6 | GY | 157 | Courtesy Lamp Control
7 | RD/WH | 1340 | Battery Positive Voltage | 7 | RD/WH | 1340 | Battery Positive Voltage
8 | BN | 201 | Left Front Speaker Output (+) (UW6) | 8 | BN | 201 | Left Front Speaker Output (+)
9 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference (UV8) | 9 | PU/WH | 659 | Cellular Telephone Voice Low Reference (NQU)
10 | D-BU | 658 | Cellular Telephone Voice Signal (UV8) | 10 | PU/WH | 658 | Cellular Telephone Voice Signal (NQU)

### X211 Front Harness to Floor Harness

#### Connector Part Information

- OEM: MG 612243-3
- Service: N/A
- Description: 15-Way F 090-II Series, KET (YE)

#### Connector Part Information

- OEM: MG 622244-3
- Service: N/A
- Description: 15-Way M 090-II Series, KET (YE)

#### X211 Front Harness to Floor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
2 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 2 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
3 | L-GN/BK | 580 | Battery Positive Voltage | 3 | L-GN/BK | 580 | Battery Positive Voltage (AE3)
4 | L-BU | 20 | Stop Lamp Supply Voltage (JM4) | 4 | L-BU | 20 | Stop Lamp Supply Voltage (JM4)
5 | BN | 1723 | Fuel Pump Relay Output | 5 | BN | 1723 | Fuel Pump Relay Output
6 | L-GN/BK | 392 | Rear Window Washer Pump Control (LHD+HB) | 6 | L-GN/BK | 392 | Rear Window Washer Pump Control (LHD+HB)
7 | PK | 539 | Ignition 1 Voltage (LHD) | 7 | PK | 539 | Ignition 1 Voltage (LHD+NB)
PK | 1739 | Ignition 1 Voltage (LHD+HB)
D-BU | 732 | Evaporator Temperature Sensor Signal (RHD) | D-BU | 732 | Evaporator Temperature Sensor Signal (RHD)
8 | PK | 639 | Ignition 1 Voltage (LHD+HB) | 8 | PK | 639 | Ignition 1 Voltage (LHD+HB)
L-BU | 733 | Low Reference (RHD) | L-BU | 733 | Low Reference (RHD)
9 | L-GN/BK | 580 | Battery Positive Voltage | 9 | L-GN/BK | 580 | Battery Positive Voltage (AE3/A32)
10 | BN | 882 | Right Rear Wheel Speed Sensor Signal (JM4) | 10 | BN | 882 | Right Rear Wheel Speed Sensor Signal (JM4)
11 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JM4) | 11 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JM4)
12 | BN | 884 | Left Rear Wheel Speed Sensor Signal (JM4) | 12 | BN | 884 | Left Rear Wheel Speed Sensor Signal (JM4)
13 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JM4) | 13 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JM4)
14 | BN/WH | 309 | Right Park Lamp Supply Voltage | 14 | BN/WH | 309 | Right Park Lamp Supply Voltage
15 | PU | 709 | Left Park Lamp Supply Voltage | 15 | PU | 709 | Left Park Lamp Supply Voltage

### X212 I/P Harness to Floor Harness (LHD)

#### Connector Part Information

- OEM: MG 651525-2
- Service: N/A
- Description: 11-Way F 090-II Series, KET (BU)

#### Connector Part Information

- OEM: MG 641528-2
- Service: N/A
- Description: 11-Way M 090-II Series, KET (BU)

#### X212 I/P Harness to Floor Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD | 1093 | Rear Defog Element Supply Voltage | 1 | RD | 1093 | Rear Defog Element Supply Voltage
2 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | 2 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
3 | RD/WH | 640 | Battery Positive Voltage | 3 | RD/WH | 640 | Battery Positive Voltage
4 | YE | 143 | Accessory Voltage | 4 | YE | 143 | Accessory Voltage
5 | GY | 393 | Rear Window Wiper Motor Control (Hatchback) | 5 | GY | 393 | Rear Window Wiper Motor Control (Hatchback)
PK/BK | 6434 | Class 2 Serial Data - Hi (Notchback+UY4) | PK/BK | 6434 | Class 2 Serial Data - Hi (Notchback+UY4)
6 | D-BU | 58 | Rear Wiper Auto Stop Signal (Hatchback) | 6 | D-BU | 58 | Rear Wiper Auto Stop Signal (Hatchback)
GY/BK | 6435 | Class 2 Serial Data - Low (Notchback+UY4) | GY/BK | 6435 | Class 2 Serial Data - LoW (Notchback+UQN)
7 | L-GN | 24 | Backup Lamp Supply Voltage (-WHB) | 7 | L-GN | 24 | Backup Lamp Supply Voltage (-WHB)
BN | 841 | Ignition 3 Voltage (WHB) | BN | 841 | Ignition 3 Voltage (WHB)
8 | GY/BK | 1501 | Driver Heated Seat High/Low Signal (C37) | 8 | GY/BK | 1501 | Driver Heated Seat High/Low Signal (C37)
RD/WH | 240 | Battery Positive Voltage (UE1) | RD/WH | 240 | Battery Positive Voltage (UE1)
9 | BN | 253 | Trunk Release Relay Control (UA5) | 9 | BN | 253 | Trunk Release Relay Control (UA5)
10 | RD/WH | 1340 | Battery Positive Voltage | 10 | RD/WH | 1340 | Battery Positive Voltage
11 | L-BU | 20 | Stop Lamp Supply Voltage | 11 | L-BU | 20 | Stop Lamp Supply Voltage

### X212 I/P Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 612243-3
- Service: N/A
- Description: 15-Way F ASC Series, KET (YE)

#### Connector Part Information

- OEM: MG 622244-3
- Service: N/A
- Description: 15-Way M ASC Series, KET (YE)

#### X212 I/P Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | 639 | Ignition 1 Voltage | 1 | PK | 639 | Ignition 1 Voltage
2 | D-GN/WH | 1317 | Front Fog Relay Control | 2 | D-GN/WH | 1317 | Front Fog Relay Control
D-GN/WH | 1317
3 | PK | 539 | Power Window Relay Output | 3 | PK | 539 | Power Window Relay Output
4 | BN | 96 | Cigar Relay Control | 4 | BN | 96 | Cigar Relay Control
5 | D-GN | 189 | Dome Relay Control | 5 | D-GN | 189 | Dome Relay Control
6 | YE | 712 | HI Beam Indicator Control | 6 | YE | 712 | HI Beam Indicator Control
7 | WH | 1080 | Illumination Relay Control | 7 | WH | 1080 | Illumination Relay Control
8 | PU | 638 | Not Used | 8 | PU | 638 | Not Used
9 | BN/WH | 309 | Illumination Relay Output | 9 | BN/WH | 309 | Illumination Relay Output
10 | D-GN | 95 | Front Wiper High Speed | 10 | D-GN | 95 | Front Wiper High Speed
11 | PK | 1739 | Ignition 1 Voltage | 11 | PK | 1739 | Ignition 1 Voltage
12 | YE | 1769 | Front Fog Relay Output | 12 | YE | 1769 | Front Fog Relay Output
13 | PK | 94 | Ignition Voltage | 13 | PK | 94 | Ignition Voltage
PK | 94
14 | BN | 28 | Horn Relay Output | 14 | BN | 28 | Horn Relay Output
15 | PU | 92 | Front Wiper Low Speed | 15 | PU | 92 | Front Wiper Low Speed

### X213 I/P Harness to Floor Harness (LHD)

#### Connector Part Information

- OEM: MG 653033
- Service: N/A
- Description: 24-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 643030
- Service: N/A
- Description: 24-Way M 090-II Series, KET (WH)

#### X213 I/P Harness to Floor Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 710 | Class 2 Serial Data (UE1) | 1 | YE | 710 | Class 2 Serial Data (UE1)
2 | RD/WH | 540 | Battery Positive Voltage (UY4) | 2 | RD/WH | 540 | Battery Positive Voltage (UQN)
3 | GY | 157 | Courtesy Lamp Control | 3 | GY | 157 | Courtesy Lamp Control
4 | PU | 156 | Courtesy Lamp Low Control | 4 | PU | 156 | Courtesy Lamp Low Control
5 | WH | 194 | Door Unlock Control (AU3) | 5 | WH | 194 | Door Unlock Control (AU3)
6 | L-BU | 195 | Door Lock Control (AU3) | 6 | L-BU | 195 | Door Lock Control (AU3)
7 | BN | 641 | Ignition 3 Voltage | 7 | BN | 641 | Ignition 3 Voltage
8 | WH | 119 | Double Voice Speaker + (UV8) | 8 | WH | 119 | Double Voice Speaker + (UV8)
OG | 667 | Cellular Telephone Voice Signal (UE1) | OG | 667 | Cellular Telephone Voice Signal (UE1)
9 | RD/BK | 202 | Battery Positive Voltage (UV8) | 9 | RD/BK | 202 | Battery Positive Voltage (UV8)
GY | 668 | Low Reference (UE1) | GY | 668 | Low Reference (UE1)
10 | OG | 191 | Driver Folding Mirror Motor Retract Control (DL7) | 10 | OG | 191 | Driver Folding Mirror Motor Retract Control (DL7)
D-GN | 1782 | Drain Wire (UE1) | D-GN | 1782 | Drain Wire (UE1)
11 | BN | 190 | Driver Folding Mirror Motor Extend Control (DL7) | 11 | YE | 190 | Driver Folding Mirror Motor Extend Control (DL7)
D-GN | 5060 | Low Speed GMLAN Serial Data (UE1) | D-GN | 5060 | Low Speed GMLAN Serial Data (UE1)
OG | 122 | Rear Fog Lamp Supply Voltage (T9E) | OG | 122 | Rear Fog Lamp Supply Voltage (T9E)
12 | PU | 1807 | Class 2 Serial Data (Primary) (UE1) | 12 | PU | 1807 | Class 2 Serial Data (Primary) (UE1)
13 | L-GN | 24 | Backup Lamp Supply Voltage (WHB) | 13 | L-GN | 24 | Backup Lamp Supply Voltage (WHB)
14 | WH | 156 | Courtesy Lamp Low Control | 14 | WH | 156 | Courtesy Lamp Low Control
15 | BN/WH | 33 | Brake Warning Indicator Control | 15 | BN/WH | 33 | Brake Warning Indicator Control
16 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 16 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
17 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 17 | GY | 295 | Door Lock Actuator Lock Control (AU3)
18 | YE | 1578 | Fuel Temperature Signal (TNK) | 18 | YE | 1578 | Fuel Temperature Signal (TNK)
19 | OG/BK | 1031 | 5-Volt Reference (TNK) | 19 | OG/BK | 1031 | 5-Volt Reference (TNK)
20 | BN/BK | 1030 | Fuel Tank Pressure Sensor Signal (TNK) | 20 | BN/BK | 1030 | Fuel Tank Pressure Sensor Signal (TNK)
21 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference (UV8) | 21 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference (NQU)
22 | D-BU | 658 | Cellular Telephone Voice Signal (UV8) | 22 | D-BU | 658 | Cellular Telephone Voice Signal (NQU)
23 | YE | 710 | Class 2 Serial Data (UE1+WHB) | 23 | YE | 710 | Class 2 Serial Data (UE1+WHB)
24 | PU | 1807 | Class 2 Serial Data (Primary) (UE1+WHB) | 24 | PU | 1807 | Class 2 Serial Data (Primary) (UE1+WHB)
D-GN/WH | 817 | Vehicle Speed Signal (UY4)

### X213 I/P Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 651086-3
- Service: N/A
- Description: 22-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 641089-3
- Service: N/A
- Description: 22-Way F 090-II Series, KET (WH)

#### X213 I/P Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 122 | Fog Lamp Feed - Rear | 1 | OG | 122 | Fog Lamp Feed - Rear
2 | WH | 156 | Courtesy Lamp Control | 2 | WH | 156 | Courtesy Lamp Control
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | L-GN | 24 | Back-Up Lamp Feed | 4 | L-GN | 24 | Back-Up Lamp Feed
5 | RD/WH | 1340 | Battery Voltage | 5 | RD/WH | 1340 | Battery Voltage
6 | OG | 267 | Heated Mirror Element Feed | 6 | OG | 267 | Heated Mirror Element Feed
OG | 267
7 | WH | 194 | Door Lock Switch Signal | 7 | WH | 194 | Door Lock Switch Signal
8 | L-BU | 195 | Power Door Lock Relay Feed - Lock Coil | 8 | L-BU | 195 | Power Door Lock Relay Feed - Lock Coil
9 | WH | 156 | Courtesy Lamp Output | 9 | WH | 156 | Courtesy Lamp Output
10 | L-BU | 20 | Stop Lamp Feed | 10 | L-BU | 20 | Stop Lamp Feed
11 | OG | 267 | Defog Relay Output | 11 | OG | 267 | Defog Relay Output
12 | L-BU | 305 | Trunk Key Cylinder Switch Signal | 12 | PU | 305 | Trunk Key Cylinder Switch Signal
13 | PU | 265 | Door Key Lock Cylinder Switch Signal - Passenger | 13 | L-GN/RD | 265 | Door Key Lock Cylinder Switch Signal - Passenger
14 | PU | 262 | Door Key Lock Cylinder Switch Signal - Driver | 14 | BN/BK | 262 | Door Key Lock Cylinder Switch Signal - Driver
15 | BN | 253 | Trunk Release Relay Feed-Coil | 15 | BN | 253 | Trunk Release Relay Feed-Coil
16 | OG/BK | 737 | Trunk Lamp Output | 16 | GY/BK | 737 | Trunk Lamp Output
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | YE | 172 | Low Fuel Indicator Lamp Output | 18 | YE | 172 | Low Fuel Indicator Lamp Output
19 | BN/WH | 33 | Brake Warning Indicator Lamp Control | 19 | BN/WH | 33 | Brake Warning Indicator Lamp Control
20 | BN/WH | 23 | Seat Belt Switch Signal | 20 | BN/WH | 23 | Seat Belt Switch Signal
21 | GY | 90 | Power Mirror Motor Feed - Right Horizontal Motor - Left Direction | 21 | GY | 90 | Power Mirror Motor Feed - Right Horizontal Motor - Left Direction
22 | PK | 739 | Ignition 1 Voltage | 22 | PK | 739 | Ignition 1 Voltage

### X214 I/P Harness to Floor Harness (LHD)

#### Connector Part Information

- OEM: MG 653033-4
- Service: N/A
- Description: 24-Way F 090-II Series, KET (GY)

#### Connector Part Information

- OEM: MG 643030-4
- Service: N/A
- Description: 24-Way M 090-II Series, KET (GY)

#### X214 I/P Harness to Floor Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 1937 | Low Reference | 1 | L-BU | 1937 | Low Reference
2 | PU | 265 | Passenger Door Key Switch Signal (UA5) | 2 | PU | 265 | Passenger Door Key Switch Signal (UA5+Notchback)
3 | L-BU | 262 | Driver Door Key Switch Signal (UA5) | 3 | BN/BK | 262 | Driver Door Key Switch Signal (UA5)
4 | L-BU | 263 | Tamper Switch Signal (UA5) | 4 | L-BU | 263 | Tamper Switch Signal (UA5+Notchback)
5 | OG/BK | 737 | Rear Compartment Lamp Control (UA5) | 5 | BK | 737 | Rear Compartment Lamp Control (UA5+Notchback)
6 | D-GN | 145 | Antenna Relay Coil Supply Voltage (Notchback-UE1) | 6 | D-GN | 145 | Antenna Relay Coil Supply Voltage (Notchback-UE1)
7 | BN/WH | 238 | Seat Belt Switch - Left | 7 | BN/WH | 238 | Seat Belt Switch - Left
8 | BN | 201 | Left Front Speaker Output (+) | 8 | BN | 201 | Left Front Speaker Output (+)
9 | L-GN | 200 | Right Front Speaker Output (+) | 9 | L-GN | 200 | Right Front Speaker Output (+)
10 | GY | 118 | Left Front Speaker Output (-) | 10 | GY | 118 | Left Front Speaker Output (-)
11 | D-GN | 117 | Right Front Speaker Output (-) | 11 | D-GN | 117 | Right Front Speaker Output (-)
12 | RD/WH | 1340 | Battery Positive Voltage (TNK) | 12 | RD/WH | 1340 | Battery Positive Voltage (TNK)
13 | L-BU | 82 | Driver Mirror Motor Left Control (DL6) | 13 | L-BU | 82 | Driver Mirror Motor Left Control (DL6)
14 | YE | 88 | Driver Mirror Motor Up Control (DL6) | 14 | YE | 88 | Driver Mirror Motor Up Control (DL6)
15 | L-GN | 89 | Driver Mirror Motor Down Control (DL6) | 15 | L-GN | 89 | Driver Mirror Motor Down Control (DL6)
16 | WH | 81 | Driver Mirror Motor Right Control (DL6) | 16 | WH | 81 | Driver Mirror Motor Right Control (DL6)
17 | GY | 90 | Passenger Mirror Motor Left Control (DL6) | 17 | GY | 90 | Passenger Mirror Motor Left Control (DL6)
18 | D-BU | 1936 | Fuel Level Sensor Signal | 18 | D-BU | 1936 | Fuel Level Sensor Signal
19 | OG/BK | 1937 | Low Reference | 19 | OG/BK | 1937 | Low Reference
20 | YE | 172 | Low Fuel Indicator Control | 20 | YE | 172 | Low Fuel Indicator Control
21 | BN | 199 | Left Rear Speaker Output (+) | 21 | BN | 199 | Left Rear Speaker Output (+)
22 | YE | 116 | Left Rear Speaker Output (-) | 22 | YE | 116 | Left Rear Speaker Output (-)
23 | D-BU | 46 | Right Rear Speaker Output (+) | 23 | D-BU | 46 | Right Rear Speaker Output (+)
24 | L-BU | 115 | Right Rear Speaker Output (-) | 24 | L-BU | 115 | Right Rear Speaker Output (-)

### X214 I/P Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 651056-5
- Service: N/A
- Description: 10-Way F 090-II Series, KET (BK)

#### Connector Part Information

- OEM: MG 641059-5
- Service: N/A
- Description: 10-Way M 090-II Series, KET (BK)

#### X214 I/P Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 294 | Power Door Lock Motor Feed - Unlock | 1 | BN | 294 | Power Door Lock Motor Feed - Unlock
2 | L-BU | 14 | Left Turn Signal | 2 | L-BU | 14 | Left Turn Signal
3 | WH | 352 | Headlamp Relay Control | 3 | WH | 352 | Headlamp Relay Control
4 | YE | 143 | Ignition 1 Voltage | 4 | YE | 143 | Ignition 1 Voltage
5 | GY | 295 | Power Door Lock Motor Feed - Lock | 5 | GY | 295 | Power Door Lock Motor Feed - Lock
6 | D-BU | 15 | Turn Signal Lamp Feed - Right Front | 6 | D-BU | 15 | Turn Signal Lamp Feed - Right Front
7 | WH | 81 | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction | 7 | WH | 81 | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction
8 | L-GN | 89 | Power Mirror Motor Feed - Left Vertical Motor - Down Direction | 8 | L-GN | 89 | Power Mirror Motor Feed - Left Vertical Motor - Down Direction
9 | L-BU | 82 | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction | 9 | L-BU | 82 | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction
10 | YE | 88 | Power Mirror Motor Feed - Left Vertical Motor - Up Direction | 10 | YE | 88 | Power Mirror Motor Feed - Left Vertical Motor - Up Direction

### X215 Air Bag Harness to I/P Harness (C98)

#### Connector Part Information

- OEM : 368501-1
- Service: N/A
- Description: 4-Way F 070 Mulit-Lock Series, AMP (WH)

#### Connector Part Information

- OEM: 174929-1
- Service: N/A
- Description: 4-Way M 070 Mulit-Lock Series, AMP (WH)

#### X215 Air Bag Harness to I/P Harness (C98)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 6168 | Left Front Impact Sensor - High | 1 | YE | 6168 | Left Front Impact Sensor - High
2 | GY | 6169 | Left Front Impact Sensor - Low | 2 | YE/BK | 6169 | Left Front Impact Sensor - Low
3 | WH/BK | 6776 | Right Front Impact Sensor - High | 3 | BN/WH | 6776 | Right Front Impact Sensor - High
4 | D-GN/WH | 6777 | Right Front Impact Sensor - Low | 4 | L-GN | 6777 | Right Front Impact Sensor - Low

### X216 Air Bag Harness to I/P Harness

#### Connector Part Information

- OEM: 936196-1
- Service: N/A
- Description: 12-Way F 090-II Series, AMP (WH)

#### Connector Part Information

- OEM: 936207-1
- Service: N/A
- Description: 12-Way M 090-II Series, AMP (WH)

#### X216 Air Bag Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 240 | Battery Positive Voltage (WHB) | 1 | RD/WH | 240 | Battery Positive Voltage (WHB)
PK | 1739 | Battery Positive Voltage (WHB)
2 | L-BU | 2221 | Vehicle Speed Sensor Signal (-WHB) | 2 | L-BU | 2221 | Vehicle Speed Sensor Signal (-WHB)
3 | D-GN/WH | 1358 | Driver Information Center Switch Signal (-WHB) | 3 | D-GN/WH | 1358 | Driver Information Center Switch Signal (AJ3-WHB)
BK/WH | 5060 | Low Speed GMLAN Serial Data (WHB) | D-GN | 5060 | Low Speed GMLAN Serial Data (WHB)
BK/WH | 5060 | Low Speed GMLAN Serial Data (WHB)
4 | RD/WH | 1340 | Battery Positive Voltage (-WHB) | 4 | RD/WH | 1340 | Battery Positive Voltage (-WHB)
5 | YE | 234 | Seat Belt Indicator Control (-WHB) | 5 | YE | 234 | Seat Belt Indicator Control (-WHB)
6 | L-GN | 1845 | Chime Control (-WHB) | 6 | L-GN | 1845 | Chime Control (-WHB)
7 | PK | 139 | Ignition 1 Voltage | 7 | PK | 139 | Ignition 1 Voltage
8 | L-BU | 327 | SIR Serial Data (-WHB) | 8 | YE/BK | 327 | SIR Serial Data (AJ3)
9 | BN | 358 | Air Bag Indicator Control (-WHB) | 9 | BN | 358 | Air Bag Indicator Control (-WHB)
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | BN/WH | 238 | Seat Belt Switch - Left | 11 | BN/WH | 238 | Seat Belt Switch - Left
12 | D-GN/WH | 1358 | DIC Switch Signal (-WHB) | 12 | D-GN/WH | 1358 | DIC Switch Signal (-WHB)

### X217 I/P Harness to HVAC Harness (C68)

#### Connector Part Information

- OEM: MG 651006
- Service: N/A
- Description: 16-Way F 090-II 1809 Series, KET (WH)

#### Connector Part Information

- OEM: MG 641007
- Service: N/A
- Description: 16-Way M 090-II 1809 Series, KET (WH)

#### X217 I/P Harness to HVAC Harness (C68)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 92 | Windshield Wiper Motor High Speed | 1 | YE/BK | -- | Windshield Wiper Motor High Speed
2 | D-GN/WH | 817 | Vehicle Speed Signal | 2 | L-GN | -- | Vehicle Speed Signal
3 | BN/WH | 309 | Right Park Lamp Supply Voltage | 3 | D-GN/WH | -- | Right Park Lamp Supply Voltage
4 | D-GN | 230 | Instrument Panel Lamps Dimming Control | 4 | D-GN/BK | -- | Instrument Panel Lamps Dimming Control
5 | RD/WH | 540 | Battery Positive Voltage | 5 | WH/RD | -- | Battery Positive Voltage
6 | PK | 239 | Ignition 1 Voltage | 6 | YE/WH | -- | Ignition 1 Voltage
7 | WH | 193 | Rear Defog Relay Control | 7 | BN/RD | -- | Rear Defog Relay Control
8 | D-GN/WH | 762 | A/C Request Signal | 8 | YE/D-GN | -- | A/C Request Signal
9 | BK | 735 | Low Reference | 9 | D-BU/WH | -- | Low Reference
10 | YE | 61 | Outside Ambient Air Temperature Sensor Signal | 10 | D-GN/YE | -- | Outside Ambient Air Temperature Sensor Signal
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used
13 | BK | 650 | Ground | 13 | BK | -- | Ground
14 | OG | 300 | Ignition 3 Voltage | 14 | RD/WH | -- | Ignition 3 Voltage
RD/WH | -- | Ignition 3 Voltage
15 | -- | -- | Not Used | 15 | D-GN | -- | Fan Switch Signal
16 | -- | -- | Not Used | 16 | RD/YE | -- | PTC On

### X218 I/P Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 651080
- Service: N/A
- Description: 20-Way F, KET (WH)

#### Connector Part Information

- OEM: MG 641083
- Service: N/A
- Description: 20-Way M, KET (WH)

#### X218 I/P Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 1937 | Fuel Gage Sensor Signal - Right | 1 | L-BU | 1937 | Fuel Gage Sensor Signal - Right
2 | D-BU | 1936 | Fuel Gage Sensor Signal - Left | 2 | D-BU | 1936 | Fuel Gage Sensor Signal - Left
3-4 | -- | -- | Not Used | 3-4 | -- | -- | Not Used
5 | RD/WH | 640 | Battery Positive Voltage | 5 | RD/WH | 640 | Battery Positive Voltage
6 | BN | 641 | Ignition 3 Voltage | 6 | BN | 641 | Ignition 3 Voltage
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used
9 | D-GN | 145 | Power Antenna Relay Feed-Coil | 9 | D-GN | 145 | Power Antenna Relay Feed-Coil
10 | BN | 201 | Speaker Feed - Left Front | 10 | BN | 201 | Speaker Feed - Left Front
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | GY | 118 | Speaker Return - Left Front | 12 | GY | 118 | Speaker Return - Left Front
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | D-GN | 117 | Speaker Return - Right Front | 14 | D-GN | 117 | Speaker Return - Right Front
15 | L-GN | 200 | Speaker Feed - Right Front | 15 | L-GN | 200 | Speaker Feed - Right Front
16 | BN | 199 | Speaker Feed - Left Rear | 16 | BN | 199 | Speaker Feed - Left Rear
17 | YE | 116 | Speaker Return - Left Rear | 17 | YE | 116 | Speaker Return - Left Rear
18 | D-BU | 46 | Speaker Feed - Right Rear | 18 | D-BU | 46 | Speaker Feed - Right Rear
19 | L-BU | 115 | Speaker Return - Right Rear | 19 | L-BU | 115 | Speaker Return - Right Rear
20 | L-GN/BK | 311 | Headlamp Low Relay Output | 20 | L-GN/BK | 311 | Headlamp Low Relay Output

### X219 I/P Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: KET MG 651044
- Service: N/A
- Description: 8-Way F (BU)

#### Connector Part Information

- OEM: KET MG 641047
- Service: N/A
- Description: 8-Way M (BU)

#### X219 I/P Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 61 | Outside Ambient Temperature Sensor Return | 1 | YE | 61 | Outside Ambient Temperature Sensor Return
2 | L-GN | 867 | ABS Failure Indicator Lamp Output | 2 | L-GN | 867 | ABS Failure Indicator Lamp Output
3 | YE | 261 | Security Signal - Arm Alarm | 3 | YE | 261 | Security Signal - Arm Alarm
4 | BK/WH | 2051 | Serial Data | 4 | BK/WH | 2051 | Serial Data
5 | BU | 1346 | Turn Signal Lamp Feed - Right Front | 5 | BU | 1346 | Turn Signal Lamp Feed - Right Front
6 | BK | 735 | Ground | 6 | L-GN/BK | 735 | Ground
7 | RD/WH | 440 | Battery Voltage | 7 | RD/WH | 440 | Battery Voltage
8 | PK/BK | 109 | Hood Ajar Switch Signal | 8 | PK/BK | 109 | Hood Ajar Switch Signal

### X220 Front Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 651044
- Service: N/A
- Description: 22-Way F, KET (BK)

#### Connector Part Information

- OEM: MG 641047
- Service: N/A
- Description: 22-Way M, KET (BK)

#### X220 Front Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 33 | Brake Warning Indicator Lamp Output | 1 | BN | 33 | Brake Warning Indicator Lamp Output
2 | RD/WH | 440 | Battery Voltage | 2 | RD/WH | 440 | Battery Voltage
3 | PU | 638 | Power Window Enable Relay Output - N.O. Contact | 3 | PU | 638 | Power Window Enable Relay Output - N.O. Contact
4 | L-GN/BK | 311 | Headlamp Low Relay Output | 4 | L-GN/BK | 311 | Headlamp Low Relay Output
5 | WH | 352 | Headlamp Relay Control | 5 | WH | 352 | Headlamp Relay Control
6 | GN | 189 | Headlamp Leveling Motor Feed | 6 | GN | 189 | Headlamp Leveling Motor Feed
7 | YE | 61 | Outside Ambient Temperature Sensor Return | 7 | YE | 61 | Outside Ambient Temperature Sensor Return
8 | L-GN | 867 | ABS Failure Indicator Lamp Output | 8 | L-GN | 867 | ABS Failure Indicator Lamp Output
9 | PK/BK | 109 | Hood Ajar Switch Signal | 9 | PK/BK | 109 | Hood Ajar Switch Signal
10 | YE | 261 | Security Signal - Arm Alarm | 10 | YE | 261 | Security Signal - Arm Alarm
11 | L-GN/BK | 735 | Outside Ambient Temperature Sensor Signal | 11 | L-GN/BK | 735 | Outside Ambient Temperature Sensor Signal
12 | GN/WH | 1317 | Fog Lamp Relay Control | 12 | GN/WH | 1317 | Fog Lamp Relay Control
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | BN/WH | 309 | Park Lamp Feed - Right | 14 | BN/WH | 309 | Park Lamp Feed - Right
15 | L-BU | 1346 | Headlamp Relay Output - N.O. Contact | 15 | L-BU | 1346 | Headlamp Relay Output - N.O. Contact
16 | L-BU | 20 | Stop Lamp Feed | 16 | L-BU | 20 | Stop Lamp Feed
17 | BK/WH | 2051 | Serial Data | 17 | BK/WH | 2051 | Serial Data
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | WH | 1080 | Illumination Relay Control | 19 | WH | 1080 | Illumination Relay Control
20 | D-BU | 15 | Turn Signal Lamp Feed - Right Front | 20 | D-BU | 15 | Turn Signal Lamp Feed - Right Front
21 | L-BU | 14 | Turn Signal Lamp Feed - Left Front | 21 | L-BU | 14 | Turn Signal Lamp Feed - Left Front
22 | PK | 94 | Windshield Washer Signal | 22 | PK | 94 | Windshield Washer Signal

### X221 Front Harness to Floor Harness (RHD)

#### Connector Part Information

- OEM: MG 651044
- Service: N/A
- Description: 11-Way F, KET (BU)

#### Connector Part Information

- OEM: MG 641047
- Service: N/A
- Description: 11-Way M, KET (BU)

#### X221 Front Harness to Floor Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage | 1 | PK | 539 | Ignition 1 Voltage
2 | PK | 1739 | Ignition 1 Voltage | 2 | PK | 1739 | Ignition 1 Voltage
3 | YE | 1769 | Front Fog Relay output | 3 | YE | 1769 | Front Fog Relay output
4 | GN | 95 | Windshield Wiper Motor High Speed | 4 | GN | 95 | Windshield Wiper Motor High Speed
5 | PU | 92 | Windshield Wiper Motor Low Speed | 5 | PU | 92 | Windshield Wiper Motor Low Speed
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BN | 96 | Windshield Wiper Switch Signal - Pulse Delay | 7 | BN | 96 | Windshield Wiper Switch Signal - Pulse Delay
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | 28 | Horn Relay Output | 9 | BN | 28 | Horn Relay Output
10 | YE | 712 | HI Beam Indicator Control | 10 | YE | 712 | HI Beam Indicator Control
11 | PK | 639 | Ignition 1 Voltage | 11 | PK | 639 | Ignition 1 Voltage

### X222 Cigar Lighter Harness to I/P Harness

#### Connector Part Information

- OEM: MG 612034
- Service: N/A
- Description: 3-Way F ASC Series, KET (WH)

#### Connector Part Information

- OEM: MG 622035
- Service: N/A
- Description: 3-Way M ASC Series, KET (WH)

#### X222 Cigar Lighter Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 650 | Ground | 2 | BK | 650 | Ground
3 | YE | 143 | Accessory Voltage | 3 | YE | 143 | Accessory Voltage

### X223 I/P Harness to APP Jumper

#### Connector Part Information

- OEM: MG 641044
- Service: N/A
- Description: 6-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 641647
- Service: N/A
- Description: 6-Way M 090-II Series, KET (WH)

#### X223 I/P Harness to APP Jumper

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | 1161 | APP Sensor 2 Signal | 1 | YE/RD | 1161 | APP Sensor 2 Signal
2 | BN | 718 | Low Reference | 2 | D-GN | 718 | Low Reference
3 | GY | 596 | 5-Volt Reference | 3 | GY | 596 | 5-Volt Reference
4 | GY | 474 | 5-Volt Reference | 4 | D-BU | 474 | 5-Volt Reference
5 | OG/BK | 645 | Low Reference | 5 | RD | 645 | Low Reference
6 | L-BU | 1162 | APP Sensor 1 Signal | 6 | YE | 1162 | APP Sensor 1 Signal

### X351 Floor Harness to Driver Door Harness

#### Connector Part Information

- OEM: MG 610692
- Service: N/A
- Description: 29-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 620693
- Service: N/A
- Description: 29-Way M 090-II Series, KET (WH)

#### X351 Floor Harness to Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/BK | 580 | Battery Positive Voltage (A32/AE3) | 1 | L-GN/BK | 580 | Battery Positive Voltage (A32/AE3)
2 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3) | 2 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3)
3 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A32/AE3) | 3 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A32/AE3)
4 | BN | 167 | Power Window Master Switch Right Front Down Signal (A32/AE3) | 4 | BN | 167 | Power Window Master Switch Right Front Down Signal (A32/AE3)
5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (AE3) | 5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (AE3)
6 | PU | 169 | Power Window Master Switch Left Rear Down Signal (AE3) | 6 | PU | 169 | Power Window Master Switch Left Rear Down Signal (AE3)
7 | BK | 650 | Ground | 7 | BK | 650 | Ground
8 | L-GN/BK | 580 | Battery Positive Voltage (A32/AE3) | 8 | L-GN/BK | 580 | Battery Positive Voltage (A32/AE3)
9 | YE | 88 | Driver Mirror Motor Up Control (DL6) | 9 | YE | 88 | Driver Mirror Motor Up Control (DL6)
10 | GY | 90 | Passenger Mirror Motor Left Control (DL6) | 10 | GY | 90 | Passenger Mirror Motor Left Control (DL6)
11 | L-BU | 82 | Driver Mirror Motor Left Control (DL6) | 11 | L-BU | 82 | Driver Mirror Motor Left Control (DL6)
12 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (DL6) | 12 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (DL6)
13 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A32/AE3) | 13 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A32/AE3)
14 | PU | 171 | Power Window Master Switch Right Rear Down Signal (A32/AE3) | 14 | PU | 171 | Power Window Master Switch Right Rear Down Signal (A32/AE3)
15 | RD/WH | 1340 | Battery Positive Voltage (UA5) | 15 | RD/WH | 1340 | Battery Positive Voltage (UA5)
16 | BN | 253 | Trunk Release Relay Control (Notchback+UA5) | 16 | BN | 253 | Trunk Release Relay Control (Notchback+UA5)
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | BN/BK | 262 | Driver Door Key Switch Signal (UA5) | 18 | L-GN/RD | 262 | Driver Door Key Switch Signal (UA5)
19 | GY | 118 | Left Front Speaker Output (-) (LHD) | 19 | GY | 118 | Left Front Speaker Output (-)
GY | 118 | Left Front Speaker Output (-) (LHD)
D-GN | 117 | Right Front Speaker Output (-) (RHD)
20 | BN | 201 | Left Front Speaker Output (+) (LHD) | 20 | BN | 201 | Left Front Speaker Output (+)
BN | 201 | Left Front Speaker Output (+) (LHD)
L-GN | 200 | Right Front Speaker Output (+) (RHD)
21 | WH | 119 | Mode Door Control (UAX) | 21 | WH | 119 | Mode Door Control (UAX)
22 | GY | 202 | Battery Positive Voltage (UAX) | 22 | RD/BK | 202 | Battery Positive Voltage (UAX)
23 | -- | -- | Not Used | 23 | -- | -- | Not Used
24 | WH | 194 | Door Unlock Control (AU3) | 24 | WH | 194 | Door Unlock Control (AU3)
25 | L-BU | 195 | Door Lock Control (AU3) | 25 | L-BU | 195 | Door Lock Control (AU3)
26 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 26 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
27 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 27 | GY | 295 | Door Lock Actuator Lock Control (AU3)
28 | L-BU | 191 | Driver Folding Mirror Motor Retract Control (DM4) | 28 | L-BU | 191 | Driver Folding Mirror Motor Retract Control (DM4)
29 | YE | 190 | Driver Folding Mirror Motor Extend Control (DM4) | 29 | YE | 190 | Driver Folding Mirror Motor Extend Control (DM4)

### X361 Floor Harness to Passenger Door Harness

#### Connector Part Information

- OEM: MG 610692
- Service: N/A
- Description: 29-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 620693
- Service: N/A
- Description: 29-Way M 090-II Series, KET (WH)

#### X361 Floor Harness to Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3) | 1 | D-BU | 1307 | Power Window Master Switch Lockout Signal (A32/AE3)
L-GN/BK | 580 | Battery Positive Voltage (A32)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A32/AE3) | 3 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A32/AE3)
4 | BN | 167 | Power Window Master Switch Right Front Down Signal (A32/AE3) | 4 | PU | 167 | Power Window Master Switch Right Front Down Signal (A32/AE3)
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | BK | 450 | Ground | 7 | BK | 650 | Ground
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-GN | 89 | Driver Mirror Motor Down Control (DL6/DM7) | 9 | L-GN | 89 | Driver Mirror Motor Down Control (DL6/DM7)
10 | GY | 90 | Passenger Mirror Motor Left Control (DL6/DM7) | 10 | GY | 90 | Passenger Mirror Motor Left Control (DL6/DM7)
11 | WH | 81 | Driver Mirror Motor Right Control (DL6/DM7) | 11 | WH | 81 | Driver Mirror Motor Right Control (DL6/DM7)
12 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (DL6/DM7) | 12 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (DL6/DM7)
13-17 | -- | -- | Not Used | 13-17 | -- | -- | Not Used
18 | L-GN/RD | 265 | Passenger Door Key Switch Signal (UA5) | 18 | L-GN/RD | 265 | Passenger Door Key Switch Signal (UA5)
19 | D-GN | 117 | Right Front Speaker Output (-) (LHD) | 19 | GY | 177 | Speaker Return
GY | 118 | Left Front Speaker Output (-) (RHD)
20 | L-GN | 200 | Right Front Speaker Output (+) (LHD) | 20 | L-GN | 200 | Speaker Feed
BN | 201 | Left Front Speaker Output (+) (RHD)
21-25 | -- | -- | Not Used | 21-25 | -- | -- | Not Used
26 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 26 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
27 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 27 | GY | 295 | Door Lock Actuator Lock Control (AU3)
28 | L-BU | 5023 | Passenger Folding Mirror Motor Retract Control (DL7) | 28 | L-BU | 5023 | Passenger Folding Mirror Motor Retract Control (DM4)
29 | WH | 5004 | Passenger Folding Mirror Motor Extend Control (DL7) | 29 | YE | 5004 | Passenger Folding Mirror Motor Extend Control (DM4)

### X371 Floor Harness to Left Rear Door Harness

#### Connector Part Information

- OEM: MG 6612228
- Service: N/A
- Description: 6-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 622229
- Service: N/A
- Description: 6-Way M 090-II Series, KET (WH)

#### X371 Floor Harness to Left Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 1 | GY | 295 | Door Lock Actuator Lock Control (AU3)
2 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 2 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
3 | PU | 171 | Power Window Master Switch Right Rear Down Signal (AE3) | 3 | PU | 171 | Power Window Master Switch Right Rear Down Signal (AE3)
4 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (AE3) | 4 | D-GN | 170 | Power Window Master Switch Right Rear Up Signal (AE3)
5 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3) | 5 | D-BU | 1307 | Power Window Master Switch Lockout signal (AE3)
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X381 Floor Harness to Right Rear Door Harness

#### Connector Part Information

- OEM: MG 6612228
- Service: N/A
- Description: 6-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 622229
- Service: N/A
- Description: 6-Way M 090-II Series, KET (WH)

#### X381 Floor Harness to Right Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 1 | GY | 295 | Door Lock Actuator Lock Control (AU3)
2 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 2 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
3 | PU | 171 | Power Window Master Switch Right Rear Down Signal (AE3) | 3 | PU | 171 | Power Window Master Switch Right Rear Down Signal (AE3)
4 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (AE3) | 4 | D-GN | 170 | Power Window Master Switch Right Rear Up Signal (AE3)
5 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3) | 5 | D-BU | 1307 | Power Window Master Switch Lockout Signal (AE3)
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X401 Tailgate Harness to Floor Harness (Hatchback)

#### Connector Part Information

- OEM: MG 610402
- Service: N/A
- Description: 8-Way F 090-II Series Sealed, KET (WH)

#### Connector Part Information

- OEM: MG 620403
- Service: N/A
- Description: 8-Way M 090-II Series Sealed, KET (WH)

#### X401 Tailgate Harness to Floor Harness (Hatchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 1093 | Rear Defog Element Supply Voltage | 2 | RD | 1093 | Rear Defog Element Supply Voltage
3 | L-BU | 20 | Stop Lamp Supply Voltage (TS6) | 3 | L-BU | 20 | Stop Lamp Supply Voltage
4 | BN | 294 | Door Lock Actuator Unlock Control (AU3) | 4 | BN | 294 | Door Lock Actuator Unlock Control (AU3)
5 | GY | 295 | Door Lock Actuator Lock Control (AU3) | 5 | GY | 295 | Door Lock Actuator Lock Control (AU3)
6 | BK | 737 | Rear Compartment Lamp Control | 6 | BK | 737 | Rear Compartment Lamp Control
7 | L-BU | 263 | Tamper Switch Signal (UA5) | 7 | L-BU | 263 | Tamper Switch Signal (UA5)
8 | BK | 850 | Ground | 8 | BK | 850 | Ground

### X401 Floor Harness to Trunk Harness (Notchback)

#### Connector Part Information

- OEM: MG 651050
- Service: N/A
- Description: 8-Way F Series Sealed, KET (WH)

#### Connector Part Information

- OEM: MG 641053
- Service: N/A
- Description: 8-Way M Series Sealed, KET (WH)

#### X401 Floor Harness to Trunk Harness (Notchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | PU | 309 | Right Park Lamp Supply Voltage
2 | L-GN | 24 | Backup Lamp Supply Voltage | 2 | L-GN | 24 | Backup Lamp Supply Voltage
L-GN | 24 | Backup Lamp Supply Voltage
3 | OG | 122 | Roof Off-Road Lamps Supply Voltage 1 (TRA) | 3 | OG | 122 | Roof Off-Road Lamps Supply Voltage 1 (TRA)
OG | 122 | Roof Off-Road Lamps Supply Voltage 1 (TRA)
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU | 709 | Left Park Lamp Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
7 | L-BU | 20 | Stop Lamp Supply Voltage | 7 | L-BU | 20 | Stop Lamp Supply Voltage
8 | BN | 841 | Ignition 3 Voltage (WHB) | 8 | BN | 841 | Ignition 3 Voltage (WHB)
BN | 841 | Ignition 3 Voltage (WHB)

### C402 Tailgate Harness to Floor Harness (Hatchback)

#### Connector Part Information

- OEM: MG 610396
- Service: N/A
- Description: 4-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 620397
- Service: N/A
- Description: 4-Way M 090-II Series, KET (WH)

#### C402 Tailgate Harness to Floor Harness (Hatchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/BK | 392 | Rear Window Washer Pump Control | 1 | L-GN/BK | 392 | Rear Window Washer Pump Control
2 | PK | 639 | Ignition 1 Voltage | 2 | PK | 639 | Ignition 1 Voltage
3 | L-BU | 393 | Rear Window Wiper Motor Control | 3 | GY | 393 | Rear Window Wiper Motor Control
4 | D-BU | 58 | Right Cornering Lamp Supply Voltage | 4 | D-BU | 58 | Right Cornering Lamp Supply Voltage

### X402 Trunk Lid Harness to Floor Harness (Notchback)

#### Connector Part Information

- OEM: MG 651044
- Service: N/A
- Description: 6-Way F 090-II Series, KET (WH)

#### Connector Part Information

- OEM: MG 641047
- Service: N/A
- Description: 6-Way M 090-II Series, KET (WH)

#### X402 Trunk Lid Harness to Floor Harness (Notchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 253 | Trunk Release Relay Control (UA5) | 1 | BN | 253 | Trunk Release Relay Control (UA5)
2 | L-BU | 20 | Stop Lamp Supply Voltage (T43) | 2 | L-BU | 20 | Stop Lamp Supply Voltage (T43)
3 | PU | 709 | Left Park Lamp Supply Voltage | 3 | PU | 709 | Left Park Lamp Supply Voltage
4 | L-BU | 263 | Tamper Switch Signal (UA5) | 4 | L-BU | 263 | Tamper Switch Signal (UA5)
5 | GY/BK | 737 | Rear Compartment Lamp Control | 5 | GY/BK | 737 | Rear Compartment Lamp Control
6 | BK | 450 | Ground | 6 | BK | 850 | Ground

### X403 Tailgate Extension Harness to Tailgate Harness (Hatchback)

#### Connector Part Information

- OEM: MG 630680
- Service: N/A
- Description: 4-Way F 090 (2.3 mm) Series, KET (WH)

#### Connector Part Information

- OEM: MG 620160
- Service: N/A
- Description: 4-Way M 090 (2.3 mm) Series, KET (WH)

#### X403 Tailgate Extension Harness to Tailgate Harness (Hatchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | OG/BK | 737 | Rear Compartment Lamp Control | 2 | OG/BK | 737 | Rear Compartment Lamp Control
3 | BK | 850 | Ground | 3 | BK | 850 | Ground
4 | L-BU | 263 | Tamper Switch Signal (UA5) | 4 | L-BU | 263 | Tamper Switch Signal (UA5)

### X404 Tailgate Harness to Tailgate Extension Harness (Hatchback)

#### Connector Part Information

- OEM: MG 610396
- Service: N/A
- Description: 4-Way F 090 (2.3 mm) Series, KET (WH)

#### Connector Part Information

- OEM: MG 620397
- Service: N/A
- Description: 4-Way M 090 (2.3 mm) Series, KET (WH)

#### X404 Tailgate Harness to Tailgate Extension Harness (Hatchback)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 393 | Rear Window Wiper Motor Control | 1 | GY | 393 | Rear Window Wiper Motor Control
2 | PK | 639 | Ignition 1 Voltage | 2 | PK | 639 | Ignition 1 Voltage
3 | L-GN/BK | 392 | Rear Window Washer Pump Control | 3 | L-GN/BK | 392 | Rear Window Washer Pump Control (C16)
4 | D-BU | 58 | Right Cornering Lamp Supply Voltage | 4 | D-BU | 58 | Right Cornering Lamp Supply Voltage (C25)

### X405 Floor Harness to Left Tail Lamp Jumper (Hatchback without T9E)

#### Connector Part Information

- OEM: MG 610152
- Service: N/A
- Description: 6-Way F 090 (2.3 mm) Series, KET (NA)

#### Connector Part Information

- OEM: MG 620153
- Service: N/A
- Description: 6-Way M 090 (2.3 mm) Series, KET (NA)

#### X405 Floor Harness to Left Tail Lamp Jumper (Hatchback without T9E)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN | 24 | Backup Lamp Supply Voltage (WHB) | 1 | BK | 24 | Backup Lamp Supply Voltage (WHB)
BK | 450 | Ground (-WHB) | BK | 450 | Ground (-WHB)
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
BK/YE | 450 | Ground
3 | BN | 841 | Ignition 3 Voltage (WHB) | 3 | WH | 841 | Ignition 3 Voltage (WHB)
L-GN | 24 | Backup Lamp Supply Voltage (-WHB) | L-GN | 24 | Backup Lamp Supply Voltage (-WHB)
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | D-BU | 709 | Left Park Lamp Supply Voltage
6 | L-BU | 20 | Stop Lamp Supply Voltage | 6 | RD | 20 | Stop Lamp Supply Voltage

### X406 Floor Harness to Right Tail Lamp Jumper (Hatchback without T9E)

#### Connector Part Information

- OEM: MG 610152
- Service: N/A
- Description: 6-Way F 090 (2.3 mm) Series, KET (NA)

#### Connector Part Information

- OEM: MG 620153
- Service: N/A
- Description: 6-Way M 090 (2.3 mm) Series, KET (NA)

#### X406 Floor Harness to Right Tail Lamp Jumper (Hatchback without T9E)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN | 24 | Backup Lamp Supply Voltage (WHB) | 1 | BK | 24 | Backup Lamp Supply Voltage (WHB)
BK | 450 | Ground (-WHB) | BK | 450 | Ground (-WHB)
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
BK/YE | 450 | Ground
3 | BN | 841 | Ignition 3 Voltage (WHB) | 3 | WH | 841 | Ignition 3 Voltage (WHB)
L-GN | 24 | Backup Lamp Supply Voltage (-WHB) | L-GN | 24 | Backup Lamp Supply Voltage (-WHB)
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Right Turn Signal Lamps Supply Voltage
5 | BN/WH | 309 | Right Park Lamp Supply Voltage | 5 | D-BU | 309 | Right Park Lamp Supply Voltage
6 | L-BU | 20 | Stop Lamp Supply Voltage | 6 | RD | 20 | Stop Lamp Supply Voltage