For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the lower steering column cover panel screws (6, 7, 8).
3. Turn the steering wheel in order to access the upper steering column cover panel screws (3, 4). Remove the upper steering column cover panel screws.
4. Remove the upper steering column cover panel (1) and the lower steering column cover panel (5).
5. Remove the turn signal switch by pushing in on the tabs (2, 3) on either side of the switch housing.
6. Disconnect the electrical connectors (1, 4) from the turn signal switch.

### Installation Procedure

1. Connect the electrical connectors (1, 4) to the turn signal switch.
2. Install the turn signal switch into the switch housing.
3. Install the upper steering column cover panel (1) and the lower steering column cover panel (5).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the lower steering column cover panel screws (6, 7, 8) and tighten to 3 N·m (27 lb in).
5. Turn the steering wheel in order to access the upper steering column cover panel screw holes. Install the upper steering column cover panel screws (3, 4) and tighten to 3 N·m (27 lb in).
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.