For 1990-2009 cars

## Radio Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the audio system trim molding.
3. Remove the screws and the audio system.
4. Disconnect the audio system electrical connector and the antenna cable.

### Installation Procedure

1. Connect the audio system electrical connector and the antenna cable.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the audio system with the screws.

Tighten
Tighten the audio system screws to 6 N·m (53 lb in).

3. Install the audio system trim molding.
4. Connect the negative battery cable.
5. Enter the audio security system 4-digit code. Refer to Radio/Audio System Description and Operation .

## Radio Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel (I/P) lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement .
3. Remove the screws and the audio system.
4. Disconnect the audio system electrical connector and the antenna cable.

### Installation Procedure

1. Connect the audio system electrical connector and the antenna cable.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the audio system with the screws.

Tighten
Tighten the audio system screws to 6 N·m (53 lb in).

3. Install the I/P lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement .
4. Connect the negative battery cable.