For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the windshield pillar garnish molding. Refer to Windshield Pillar Garnish Molding Replacement.
3. Disconnect the electrical connector.
4. Remove the tweeter.

### Installation Procedure

1. Install the tweeter.
2. Connect the electrical connector.
3. Install the windshield pillar garnish molding. Refer to Windshield Pillar Garnish Molding Replacement.
4. Connect the negative battery cable.