For 1990-2009 cars

## Horn Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the left headlamp assembly. Refer to Headlamp Replacement .
3. Remove the bolt from the horn.
4. Disconnect the electrical connector.
5. Remove the horn (1).

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the horn (1) with the bolt.

Tighten
Tighten the horn bolt to 21 N·m (16 lb ft).

3. Install the left headlamp assembly. Refer to Headlamp Replacement .
4. Connect the negative battery cable.

## Horn Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the fascia grille. Refer to Fascia Grille Replacement .
3. Remove the bolt from the horn.
4. Disconnect the electrical connector.
5. Remove the horn (1).

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the horn (1) with the bolt.

Tighten
Tighten the horn bolt to 21 N·m (16 lb ft).

3. Install the fascia grille. Refer to Fascia Grille Replacement .
4. Connect the negative battery cable.