For 1990-2009 cars

## Headlamp Replacement Notchback

### Removal Procedure

1. Remove the headlamp mounting bolts.
2. Disconnect the electrical connectors.
3. Remove the headlamp assembly.
4. Remove the cap concealing the headlamp bulb.
5. Disconnect the headlamp bulb electrical connector.
6. Remove the retaining wire.
7. Remove the headlamp bulb.

### Installation Procedure

1. Install the headlamp bulb.
2. Install the retaining wire.
3. Connect the headlamp bulb electrical connector.
4. Install the cap concealing the headlamp bulb.
5. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the headlamp assembly with the bolts.

Tighten
Tighten the headlamp assembly bolts to 6 N·m (53 lb in).

## Headlamp Replacement Hatchback

### Removal Procedure

1. Remove the headlamp mounting bolts.
2. Disconnect the electrical connectors.
3. Remove the headlamp assembly.
4. Remove the cap concealing the headlamp bulb.
5. Disconnect the headlamp bulb electrical connector.
6. Remove the retaining wire.
7. Remove the headlamp bulb.

### Installation Procedure

1. Install the headlamp bulb.
2. Install the retaining wire.
3. Connect the headlamp bulb electrical connector.
4. Install the cap concealing the headlamp bulb.
5. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the headlamp assembly with the bolts.

Tighten
Tighten the headlamp assembly bolts to 6 N·m (53 lb in).