For 1990-2009 cars

### Removal Procedure

1. Remove the camshaft adjuster bolts (3).

Note: Ensure the location and direction of the intake/exhaust adjusters when removed.

2. Remove the camshaft adjusters (1, 2).

### Installation Procedure

Note: Ensure the location and direction of the intake/exhaust adjusters when removed.

1. Install the camshaft adjusters (1, 2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the camshaft adjuster bolts (3) and tighten to 65 N·m +120° +15° (47.9 lb ft +120° +15° ).