For 1990-2009 cars

### Draining Procedure

Caution: Refer to Vehicle Lifting and Jacking Caution in the Preface section.

1. Raise and support the vehicle.
2. Place a suitable fluid drainage container under the transaxle.
3. Remove the fluid drain plug. Allow the fluid to drain completely.
4. Clean the drain plug threads.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the fluid drain plug and tighten to 17 N·m (13 Ib ft).

### Filling Procedure

1. Remove the drainage container and lower the vehicle.
2. Add 3/4 of the recommended amount of T-IV Automatic Transmission Fluid.
3. Start the engine and allow it to reach normal operating temperature.
4. Shift the gear selector through all positions.

Note: The correct fluid level must be between the HOT MIN (2) and the HOT MAX (1) notches on the dipstick.

5. Check the fluid level and add fluid until the dipstick indicates the proper level.