For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the EVAP canister vent solenoid valve connector.
3. Disconnect the EVAP canister vent hose.
4. Remove the EVAP canister vent assembly (1) pushing it to the left side.

### Installation Procedure

1. Install the EVAP canister vent assembly (1) pushing it to the right side.
2. Connect the EVAP canister vent hose.
3. Connect the EVAP canister vent solenoid valve connector.
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.