For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the blower motor electrical connector.
3. Remove the blower cooling hose.
4. Remove the screws that secure the motor to the heater/air distribution case.
5. Remove the motor and the seal from the heater/air distribution case by gently pulling the motor straight down and out.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the blower motor and seal, with the shock mount pads, in the heater/air distribution case. Hold the blower motor in position.
2. Install the screws to secure the blower motor to the heater/air distribution case.

Tighten
Tighten the blower motor retaining screws to 6 N·m (53 lb in).

3. Install the blower motor cooling hose.
4. Connect the electrical connector.
5. Connect the negative battery cable.
6. Confirm that the blower motor operates properly.