For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Support the engine assembly using DW-110-060 support fixture .
3. Remove the engine mount bracket retaining bolts (2)/nuts (1).
4. Remove the engine mount retaining bolts (2).
5. Remove the engine mount assembly (1).

### Installation Procedure

1. Install the engine mount assembly (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the engine mount retaining bolts (2).

Tighten
Tighten the engine mount retaining bolts to 55 N·m (40.5 lb ft).

3. Tighten the engine mount bracket retaining bolts (2)/nuts (1).

Tighten
Tighten the engine mount bracket retaining bolts/nuts to 65 N·m (47.9 lb ft).

4. Remove the DW-110-060 support fixture .
5. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.