For 1990-2009 cars

### Removal Procedure

1. Remove the front door escutcheon. Manual remote control mirror shown.
2. Disconnect the electric control rearview mirror electrical connector, if equipped.
3. Remove the screws and the outside rearview mirror assembly from the door. Manual remote control mirror shown.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outside rearview mirror assembly screws. Manual remote control mirror shown.

Tighten
Tighten the outside rearview mirror assembly screws to 4.5 N·m (40 lb in).

2. Connect the electric control rearview mirror electrical connector, if equipped.
3. Install the escutcheon. Manual remote control mirror shown.