For 1990-2009 cars

### Disassemble Procedure

#### Special Tools

• | J 8062 Universal Valve Spring Compressor

• | EN-46119 Valve Spring Compressing Adapter

1. Remove the camshaft position solenoid valve housing.
2. Remove the camshaft cap bolts in this sequence (1)-(4)-(2)-(3).
3. Remove the camshaft caps.
4. Remove the camshafts (1, 2)and oil seal rings (3).
5. Remove the valve tappet.
6. Install the J 8062 Universal Valve Spring Compressor and EN-46119 Valve Spring Compressing Adapter .
7. Remove the valve key.
8. Remove the valves (5), springs (3), retainers (2), and seals (4).