For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Belt Tensioner Bolt | 50 N·m | 36.8 lb ft
Alternator B+ Tightening Nut | 15 N·m | 11 lb ft
Camshaft Adjuster Bolts | 65 N·m + 120° + 15° | 47.9 lb ft + 120° + 15°
Camshaft Bearing Cap Bolts | 8 N·m | 70.8 lb in
Camshaft Sprocket Bolt Cap | 50 N·m | 36.8 lb ft
Camshaft Sprocket Bolts | 65 N·m | 47.9 lb ft
Closure Bolt | 15 N·m | 11 lb ft
Connecting-rod Caps Bolts | 35 N·m + 45° +15° | 25.8 lb ft +45° +15°
Coolant Pipe To Coolant Distributor Case Bolts | 8 N·m | 70.8 lb in
Crankshaft Cap Bolts | 50 N·m + 50° | 36.8 lb ft + 50°
Crankshaft Pulley Bolt | 25 N·m | 18.4 lb ft
Cylinder Head Bolts | 25 N·m + 90° + 90° + 45° | 18.4 lb ft + 90° + 90° + 45°
Cylinder Head Cover Bolts | 8 N·m | 70.8 lb in
Engine Front Cover Assembly Bolts | 20 N·m | 14.7 lb ft
Engine Mount Bolts and Nuts | 55 N·m | 40.5 lb ft
Engine Mount Bracket Bolt | 65 N·m | 47.9 lb ft
Exhaust Manifold Lower Bracket Bolts | 20 N·m | 14.7 lb ft
Exhaust Manifold Nuts | 20 N·m | 14.7 lb ft
Flywheel Flexible Plate Bolts | 35 N·m+ 30° + 15° | 25.8 lb ft + 30° + 15°
Ground Tightening Nut | 12 N·m | 8.8 lb ft
Heat Exchanger Bolts | 8 N·m | 70.8 lb in
Heat Shields Bolts | 8 N·m | 70.8 lb in
Ignition Coil Bolt | 8 N·m | 70.8 lb in
Indicator Tube Tightening Bolt | 10 N·m | 7.3 lb ft
Intake Manifold Bolts | 20 N·m | 14.7 lb ft
Intake Manifold Lower Bracket Bolt | 8 N·m | 70.8 lb in
Oil Cooler Tightening Bolts | 25 N·m | 18.4 lb ft
Oil Pan Baffle Bolts | 10 N·m | 7.3 lb ft
Oil Pan Bolts | 14 N·m | 10.3 lb ft
Oil Pan-to-Transmission Bolts | 40 N·m | 29.5 lb ft
Reaction Rod-to-Bracket Bolt and Nut | 80 N·m | 59 lb ft
Reaction Rod-to-Crossmember Bolts | 55 N·m | 40.5 lb ft
Spark Plug | 25 N·m | 18.4 lb ft
Starter Solenoid B+ Tightening Nut | 10.5 N·m | 7.7 lb ft
Starter Solenoid Ground Tightening Nut | 38 N·m | 28 lb ft
Timing Belt Idler Bolt | 50 N·m | 36.8 lb ft
Timing Belt Lower Cover Bolts | 6 N·m | 53.1 lb in
Timing Belt Rear Cover Bolts | 6 N·m | 53.1 lb in
Timing Belt Tensioner Bolt | 55 N·m | 40.6 lb ft
Timing Belt Upper Cover Bolts | 4 N·m | 35.4 lb in
Transmission Tightening Bolt | 60 N·m | 44.2 lb ft