For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the windshield pillar garnish molding. Refer to Windshield Pillar Garnish Molding Replacement .
3. Disconnect the electrical connector.
4. Remove the tweeter.

### Installation Procedure

1. Install the tweeter.
2. Connect the electrical connector.
3. Install the windshield pillar garnish molding. Refer to Windshield Pillar Garnish Molding Replacement .
4. Connect the negative battery cable.