For 1990-2009 cars

#### Special Tools

J 28647-B Engine Support Fixture

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Install J 28647-B Engine Support Fixture .
3. Remove the engine mount bolts (2) and nuts (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine mount bolts (2) and nuts (1) and tighten to 55 N·m (40.5 lb ft).
2. Remove J 28647-B Engine Support Fixture .
3. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.