For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement
3. Disconnect the electrical connector.
4. Remove the retaining screws.
5. Remove the air inlet tube.
6. Remove the inside air temperature sensor.

### Installation Procedure

1. Install the inside air temperature sensor with the retaining screws and tighten.
2. Install the air inlet tube and connect the electrical connector.
3. Install instrument panel assembly. Refer to Instrument Panel Assembly Replacement
4. Connect the negative battery cable.