For 1990-2009 cars

#### Special Tools

• | EN-49074 Universal Valve Spring Compressor

• | EN-49075 Valve Spring Compressing Adapter

Note: Take extreme care to prevent any scratches, nicks or damage to the camshaft surfaces.

1. Remove the camshaft sprocket.
2. Remove the camshaft cap bolts in this sequence (1)-(4)-(2)-(3).
3. Remove the camshaft caps.
4. Remove the camshafts and oil seal rings.
5. Remove the valve tappet.
6. Install the EN-49074 compressor and EN-49075 adapter .
7. Remove the valve key.
8. Remove the valves, springs (2), retainers (1), and seals (3).